For 1990-2009 cars

# Information on Slight Vehicle Movement in Park at Start Up After Cold Soak

Subject: | Information on Slight Vehicle Movement In Park At Start Up After Cold Soak

Models: | 2009 and Prior GM Passenger Cars and Light Duty Trucks (including Saturn)

| 2009 and Prior HUMMER H2, H3

| 2009 and Prior Saab 9-7X

| with Automatic Transmission

Some vehicles may rock or move slightly forward or rearward while in park at start up after cold soak. This condition may be accompanied by a clunk noise. This is a slight movement that is more often seen visually, rather than felt, when viewed from the outside and using the auto-start feature, if equipped.

This slight movement is due to the residual transmission fluid in the clutch packs that creates a partial apply on start up. This movement is stopped by the parking pawl and/or transmission fluid exhausting completely from the clutch packs.

This slight movement has no adverse affects on the transmission and no repair should be attempted. This condition is normal. This can be verified by comparing with another identically built vehicle under the same cold conditions.

To prevent this condition from occurring, the parking brake should be utilized as per the Owner's Manual recommendations anytime the vehicle is parked.