For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Brake Hose to Caliper | 40 N·m | 30 lb ft
Brake Pipe Bracket-to-Rear Axle Control Arm | 8 N·m | 71 lb in
Brake Pipe-to-Rear Caliper | 16 N·m | 12 lb ft
Brake Rotor Retaining Screw | 4 N·m | 35 lb in
Caliper Bleeder Valve | 6 N·m | 53 lb in
Caliper-to-Bracket Guide Pins | 30 N·m | 22 lb ft
Front Brake Caliper-to-Steering Knuckle Bolts | 95 N·m | 70 lb ft
Front Brake Rotor Retaining Fastener | 4 N·m | 35 lb in
Front Brakes

- Brake Caliper Bracket Caliper-to-Steering Knuckle Bolts

95 N·m

70 lb ft

- Brake Caliper-to-Bracket Guide Pins

30 N·m

22 lb ft

- Brake Rotor Retaining Fastener

4 N·m

35 lb in

- Brake Caliper Bleeder Valve

6 N·m

53 lb in

Rear Brakes

- Brake Caliper-to-Rear Axle Control Arm Bolts

80 N·m

59 lb ft

- Brake Pipe Bracket-to-Rear Axle Control Arm

8 N·m

71 lb in

- Brake Rotor Retaining Fastener

4 N·m

35 lb in

- Brake Caliper Bleeder Valve

6 N·m

53 lb in

Rear Caliper Bleeder Valve | 6 N·m | 53 lb in
Rear Caliper-to-Rear Axle Control Arm | 80 N·m | 59 lb ft
Rear Caliper-to-Rear Axle Control Arm Bolts | 80 N·m | 59 lb ft