For 1990-2009 cars

#### Tools Required

• | J 41681 Clutch Spring Compressor

• | J 23327 Clutch Spring Compressor

1. Install new O-rings at the following locations:

• | The inner reverse brake piston

• | The reaction sleeve

• | The outer reverse brake piston

2. Lubricate the new O-rings with A/T fluid.
3. Install the following components to the transmission case:

• | The outer reverse brake piston

• | The reaction sleeve

• | The inner reverse brake piston

4. Compress the reverse brake piston using the J 41681 and the J 23327 in order to install the snap ring.