For 1990-2009 cars

## Instrument Panel Compartment Replacement SKY

Callout | Component Name
--- | ---
1 | Instrument Panel (I/P) Compartment Hinge Pin (Qty: 2)
2 | I/P Compartment Assembly

#### Procedures

1. Disconnect the compartment dampener from the compartment assembly.
2. Squeeze the sides of the compartment and pull the compartment open past the stops.

## Instrument Panel Compartment Replacement Solstice

Callout | Component Name
--- | ---
1 | Instrument Panel (I/P) Compartment Assembly

#### Procedure

Disconnect the I/P compartment damper from the I/P compartment.