For 1990-2009 cars

Connector 1: | Rear Window Defogger Grid C1
Connector 2: | Rear Window Defogger Grid C2
Connector 3: | Window Motor - Driver
Connector 4: | Window Motor - Passenger
Connector 5: | Window Switch - Driver (Early Production)
Connector 6: | Window Switch - Driver (Late Production)
Connector 7: | Window Switch - Passenger

### Rear Window Defogger Grid C1

#### Connector Part Information

- OEM: 12004267
- Service: 08911256
- Description: 1-Way F 56 Series Lock Type (BK)

#### Terminal Part Information

- Terminal: 12124515/1
- Core/Insulation Crimp: C/D
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

#### Rear Window Defogger Grid C1

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PU | 293 | Rear Defog Element Supply Voltage

### Rear Window Defogger Grid C2

#### Connector Part Information

- OEM: 12004267
- Service: 08911256
- Description: 1-Way F 56 Series Lock Type (BK)

#### Terminal Part Information

- Terminal: 12124515/1
- Core/Insulation Crimp: C/D
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

#### Rear Window Defogger Grid C2

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BK | 850 | Ground

### Window Motor - Driver

#### Connector Part Information

- OEM: 12129487
- Service: 88988609
- Description: 2-Way F Metri-Pack Series, Flexlock, Sealed (GY)

#### Terminal Part Information

- Terminal: 12110845/4
- Core/Insulation Crimp: F/5
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Window Motor - Driver

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BN | 165 | Power Window Motor Left Front Down Control
B | D-BU | 164 | Power Window Motor Left Front Up Control

### Window Motor - Passenger

#### Connector Part Information

- OEM: 12129487
- Service: 88988609
- Description: 2-Way F Metri-Pack Series, Flexlock, Sealed (GY)

#### Terminal Part Information

- Terminal: 12110845/4
- Core/Insulation Crimp: F/5
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Window Motor - Passenger

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BN | 667 | Power Window Motor Right Front Down Control
B | D-BU | 666 | Power Window Motor Right Front Up Control

### Window Switch - Driver (Early Production)

#### Connector Part Information

- OEM: 15326924
- Service: 15306174
- Description: 8-Way F GT 280 Series (BK)

#### Terminal Part Information

- Pins: A, C, D, F-H
- Terminal/Tray: 15304713/19
- Core/Insulation Crimp: Pins A, C, D, G, H - F/D
- Core/Insulation Crimp: Pin F - 4/4
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

- Pins: B
- Terminal/Tray: 15304711/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Window Switch - Driver (Early Production)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | L-BU | 166 | Power Window Master Switch Right Front Up Signal
B | GY | 8 | Instrument Panel Lamp Supply Voltage
C | D-GN | 801 | Retained Accessory Power Fuse Supply Voltage
D | TN | 167 | Power Window Master Switch Right Front Down Signal
E | -- | -- | Not Used
F | BK | 550 | Ground
G | D-BU | 164 | Power Window Motor Left Front Up Control
H | BN | 165 | Power Window Motor Left Front Down Control

### Window Switch - Driver (Late Production)

#### Connector Part Information

- OEM: 15449340
- Service: 88987856
- Description: 8-Way F GT 280 Series (BK)

#### Terminal Part Information

- Pins: A, C, D, F-H
- Terminal/Tray: 15304713/19
- Core/Insulation Crimp: Pins A, C, D, G, H - F/D
- Core/Insulation Crimp: Pin F - 4/4
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

- Pins: B
- Terminal/Tray: 15304711/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Window Switch - Driver (Late Production)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | L-BU | 166 | Power Window Master Switch Right Front Up Signal
B | GY | 8 | Instrument Panel Lamp Supply Voltage
C | D-GN | 801 | Retained Accessory Power Fuse Supply Voltage
D | TN | 167 | Power Window Master Switch Right Front Down Signal
E | -- | -- | Not Used
F | BK | 550 | Ground
G | D-BU | 164 | Power Window Motor Left Front Up Control
H | BN | 165 | Power Window Motor Left Front Down Control

### Window Switch - Passenger

#### Connector Part Information

- OEM: 12191825
- Service: 15306048
- Description: 8-Way F GT 280 Series (BN)

#### Terminal Part Information

- Pins: H
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit
- Pins: A, D, F, G
- Terminal/Tray: 15304713/19
- Core/Insulation Crimp: F/D
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)
- Pins: B, C
- Terminal/Tray: 15304711/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Window Switch - Passenger

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | D-GN | 801 | Retained Accessory Power Fuse Supply Voltage
B | GY | 8 | Instrument Panel Lamp Supply Voltage (1)
C | BK | 550 | Ground
D | TN | 167 | Power Window Master Switch Right Front Down Signal
E | -- | -- | Not Used
F | BN | 667 | Power Window Motor Right Front Down Control
G | D-BU | 666 | Power Window Motor Right Front Up Control
H | L-BU | 166 | Power Window Master Switch Right Front Up Signal