For 1990-2009 cars

Connector 1: | Clutch Start Switch (MA5)
Connector 2: | Generator

### Clutch Start Switch (MA5)

#### Connector Part Information

- OEM: 12041433
- Service: 12126463
- Description: 2-Way F Metri-Pack 280 Series (BK)

#### Terminal Part Information

- Terminal: 12034046/2
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

#### Clutch Start Switch (MA5)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PK | 339 | Ignition 1 Voltage
B | YE | 575 | Starter Control

### Generator

#### Connector Part Information

- OEM: 12186568
- Service: See Catalog
- Description: 4-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Generator

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | OG | 225 | Generator Turn On Signal
C | GY | 23 | Generator Field Duty Cycle Signal
D | -- | -- | Not Used