For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
AM/FM Radio Receiver Fasteners | 2 N·m | 18 lb in
Audio Amplifier Fasteners | 9 N·m | 80 lb in
Cellular Communication Antenna Fastener | 9 N·m | 80 lb in
Cellular Communication Microphone Fasteners | 2 N·m | 18 lb in
Communication Interface Module Bracket Fasteners | 9 N·m | 80 lb in
Communication Interface Module Fasteners | 9 N·m | 80 lb in
Digital Radio Antenna Fastener | 9 N·m | 80 lb in
Digital Radio Receiver Bracket Nut | 5 N·m | 44 lb in
Digital Radio Receiver Nut | 10 N·m | 89 lb in
Door Speaker Fasteners | 2 N·m | 18 lb in
Instrument Panel Wiring Harness Bracket Nut | 10 N·m | 89 lb in
Quarter Speaker Nut | 9 N·m | 80 lb in
Radio Antenna Bezel | 6 N·m | 53 lb in
Radio Antenna Bolt/Screw | 9 N·m | 80 lb in
Radio Bolt/Screw | 2.3 N·m | 20 lb in
Sub Woofer Box to Body Fasteners | 7 N·m | 62 lb in