For 1990-2009 cars

#### Body Control Module (BCM)

Scan Tool Output Control | Additional Menu Selection(s) | Description
--- | --- | ---
Backup Lamps | Body and Accessories/Lighting Systems/Special Functions/Light Test | The body control module (BCM) activates the backup lamps for 5 seconds when you select ON. This applies to vehicles equipped with automatic transmissions only.
Fog Lamps | Body and Accessories/Lighting Systems/Special Functions/Light Test | The BCM activates the fog lamps for 5 seconds when you select ON.
Headlamps | Body and Accessories/Lighting Systems/Special Functions/Light Test | The BCM activates the low beam headlamps for 5 seconds when you select ON.
High Beams | Body and Accessories/Lighting Systems/Special Functions/Light Test | The BCM activates the high beam headlamps for 5 seconds when you select ON.
Inadvertent Power | Body and Accessories/Lighting Systems/Special Functions/Light Test | The BCM activates the inadvertent power relay for 5 seconds when you select ON.
Interior Lamps | Body and Accessories/Lighting Systems/Special Functions/Light Test | The BCM activates the interior lamp control for 5 seconds when you select ON. The courtesy lamps should illuminate for 5 seconds and then turn off through the theater dimming feature.
LF Turn Lamp/DRL | Body and Accessories/Lighting Systems/Special Functions/Light Test | The BCM activates the left front turn/drl lamp for 5 seconds when you select ON.
LR Stop/Turn Signal Lamp | Body and Accessories/Lighting Systems/Special Functions/Light Test | The BCM activates the left rear stop/turn lamp for 5 seconds when you select ON.
Parking Lamps | Body and Accessories/Lighting Systems/Special Functions/Light Test | The BCM activates the park lamp relay for 5 seconds when you select ON.
RF Turn Lamp/DRL | Body and Accessories/Lighting Systems/Special Functions/Light Test | The BCM activates the right front turn/drl lamp for 5 seconds when you select ON.
RR Stop/Turn Signal Lamp | Body and Accessories/Lighting Systems/Special Functions/Light Test | The BCM activates the right rear stop/turn lamp for 5 seconds when you select ON.