For 1990-2009 cars

Callout | Component Name
--- | ---
Notice: Refer to Fastener Notice in the Preface section. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications .

#### Preliminary Procedure

Remove the air cleaner assembly. Refer to Air Cleaner Assembly Replacement .

1 | Stud, Air Cleaner Tighten 10 N·m (89 lb in)
2 | Nut, Radiator Upper Bracket Tighten 9 N·m (80 lb in)
3 | Bracket Assembly, Radiator Upper