For 1990-2009 cars

The following table provides the description of the Regular Production Option (RPO) codes that are available on the vehicle. The vehicle RPO list is printed on the Service Parts Identification Label.

RPO | Description
--- | ---
AF2 | Adjuster, Seat-Power, 2 Way, Vertical, Driver
AL0 | Sensor Indicator, Inflatable Restraint, Front Passenger/Child Presence Detector
AU0 | Lock Control, Entry - Remote Entry
AU3 | Lock Control - Side Door, Electric
AZ5 | Covering Headliner-Convertible Top Trim
A31 | Window - Power Operated, All Doors
A50 | Seat - Front, Bucket
B32 | Covering Front - Floor Mats, AUX
B70 | Plate-Door Sill Cover
CE7 | Certification-Emission, Exported Vehicle
CT1 | Country-Belgium
CT3 | Country-Germany
CU1 | Country-Norway
CU4 | Country-Sweden
CV3 | Country - Mexico
CW7 | Country-Puerto Rico/US Virgin Islands
C41 | HVAC System - Heater, Outside Air, with Fan
C60 | HVAC System - Air Conditioner FRT, MAN Controls
DNR | Equipment-Dealer Installed
DT4 | Ashtray-Cigarette Lighter
D44 | Mirror O/S - Color
D48 | Mirror O/S - LH & RH, Remote Control, Electric, Color
D52 | Spoiler-RR End, Sport
EXP | Export
FE2 | Suspension System, Ride, Handling
FE3 | Suspension System, Sport
FE9 | Certification - Emission, Federal
GTA | Model Conversion, Turbo
GT4 | Axle Rear - 3.73 Ratio
GW1 | Axle Rear - 3.91 Ratio
G80 | Axle Positraction - Limited Slip
JF5 | Pedals, Sporty, Alloy
JL4 | Control, Active Brake
JL9 | Brake System - PWR, FRT & RR Disc, Antilock, FRT & RR WHL
J65 | Brake System - PWR, FRT & RR DISC
KG7 | Generator - 125 AMP
KG9 | Generator - 140 AMP
K34 | Cruise Control - Automatic, Electronic
LE5 | Engine - Gas, 4 Cyl, 2.4L, MFI, ALUM, DOHC, HO, ECOTEC
LNF | Engine, Gas, 4 Cyl, 2.0L, DI, Alum, DOHC, Turbo, GM
MA5 | Transmission - Man 5 Spd, Aisin, 82 mm, 3.753 1st, 0.729 5th
MM5 | Merchandised Trans-Manual 5 Spd Provisions
MX0 | Merchandised Trans-Auto Provisions, O/D
M82 | Transmission - Auto 5 Spd, HMD, 5L40-E, Electronic
NE1 | Certification - Emission, Geographically Restricted Registration for Vehicles up to 14,000 lbs GVW (use 2003 MDL YR)
NT4 | Emission System-EEC 05
NT7 | Emission System-Federal, Tier 2
NU1 | Emission System-California, LEV2
N34 | Steering Wheel - Leather, 3 Spokes
N45 | Steering Wheel - 3 Spokes
N87 | Wheel - 18 X 8, Aluminum
PD5 | Wheel - 18 X 8, Aluminum, Chromed
QFX | Tire All - P245/45R18 - 96V BW R/PE ST TL AL3
QF8 | Wheel - 18 X 8, Aluminum, Polished
QSL | Tire All - P245/45R18 - 96W BW TL HW4
T96 | Lamp - Fog, FRT
T98 | Stamping - Vehicle Identification Number
UE1 | Communication System - Vehicle, G.P.S. 1
UK3 | Control - Steering Wheel, Accessory
UQ3 | Speaker System - Enhanced Audio
US6 | Antenna - Fixed, Painted, Radio
US8 | Radio - AM/FM Stereo, SEEK/SCAN, CD, Auto Tone, Clock, ETR, MP3, RDS
US9 | Radio - AM/FM Stereo, SEEK/SCAN, RDS, Multiple Compact Disc, Auto Tone Control, Clock, ETR, MP3
UW5 | Speaker System - 6, Base
U1C | Radio - AM/FM Stereo, SEEK/SCAN, CD, Clock, ETR
U2K | Digital Audio System - S - Band
U19 | Speedometer - Inst, Kilo & Miles, Kilo Odometer
U68 | Display - Driver Info Center
VC4 | Label - Price/Fuel Econ, Puerto Rico and Virgin Islands
VG8 | Vehicle - Label, Notice to Buyer
VH5 | Plate-Vehicle Identification
VK3 | License Plate Front - FRT Mounting PKG
VPM | Modification-Noise Control, Mexico
VY7 | Knob - Trans Cont Lever, Leather
V73 | Vehicle Statement - USA/Canada
V78 | Vehicle Statement - Delete
WIL | Plant Code-Wilmington, DE, USA
YF5 | Certification - Emission, California
Z0K | Merchandised Package-Sport Version
ZQ2 | Sales Package - Driver Convenience
ZQ3 | Sales Package - Driver Convenience II
Z49 | Export - Canadian Modif Mandatory Base Equip