For 1990-2009 cars

## Instrument Panel Insulator Panel Replacement - Right Side Sky

Callout | Component Name
--- | ---
1 | Closeout Insulator Screw Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (22 lb in)
2 | Closeout Insulator Push-in Fastener
3 | Closeout Insulator Assembly Tip Ensure the tab on the far right side of the insulator panel locks in behind the right hinge pillar trim panel.

## Instrument Panel Insulator Panel Replacement - Right Side Solstice

Callout | Component Name
--- | ---
1 | Instrument Panel Insulator Push Pin (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb ft)
2 | Instrument Panel Insulator Assembly Tip Ensure the tab on the far right side of the trim panel locks behind the right hinge pillar garnish molding.