For 1990-2009 cars

## Parking and Turn Signal Lamp Bulb Replacement SKY

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Open the hood.
2. Reach in between the bumper and front hood opening and rotate the park turn bulb socket counterclockwise a quarter turn, and remove.

1 | Park and Turn Signal Lamp Bulb Socket Tip Rotate the bulb socket counterclockwise from the lamp housing in order to remove.
2 | Park and Turn Signal Lamp Bulb Tip Push the bulb inward and rotate a quarter turn to remove the bulb from the lamp socket.

## Parking and Turn Signal Lamp Bulb Replacement Solstice

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Open the hood.
2. Reach in between the bumper and front hood opening to disconnect the turn signal and fog lamp connector, if equipped, electrical connectors.
3. Disconnect the front main harness electrical connector from the impact bar from the bulb harness.

1 | Park and Turn Signal Lamp Bulb Tip Rotate the bulb socket counterclockwise from the lamp housing in order to remove.