For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the rear compartment lid trim. Refer to Rear Compartment Lid Inner Panel Trim Replacement .

1 | Bolt, Mobile Telephone and Vehicle Location Antenna (Qty: 1) Notice: Refer to Fastener Notice in the Preface section. Tighten 9 N·m (80 lb in)
2 | Expansion Sleeve, Mobile Telephone and Vehicle Location Antenna
3 | Antenna and Base Assembly, Mobile Telephone and Vehicle Location