For 1990-2009 cars

## Torque Converter Cover Replacement Flywheel Cover

Callout | Component Name
--- | ---

#### Preliminary Procedures

Raise the vehicle. Refer to Lifting and Jacking the Vehicle .

1 | Flywheel Access Cover Bolt Notice: Refer to Fastener Notice in the Preface section. Tighten 10 N·m (89 lb in)
2 | Flywheel Access Cover

## Torque Converter Cover Replacement Torque Converter Cover

Callout | Component Name
--- | ---

#### Preliminary Procedures

Raise the vehicle. Refer to Lifting and Jacking the Vehicle .

1 | Torque Converter Access Hole Cover