For 1990-2009 cars

## Air Inlet Grille Panel Replacement SKY

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the wiper arms. Refer to Windshield Wiper Arm Replacement .

1 | Air Inlet Grille Retainer (Qty: 6)
2 | Air Inlet Grille Retainer (Qty: 4) Tip There are two retainers at each end of the air inlet grille panel.
3 | Air Inlet Grille Panel Tip Locate the rear tabs under the lower edge of the windshield prior to securing the retainers.

## Air Inlet Grille Panel Replacement Solstice

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the wiper arms. Refer to Windshield Wiper Arm Replacement .

1 | Air Inlet Grille Retainer (Qty: 10)
2 | Air Inlet Grille
3 | Washer Pump Hose Tip Disconnect at the outer edge of the air inlet grille panel.