For 1990-2009 cars

When you open the hood on the 2.4L L4 engine, this is what you will see:

1. Windshield Washer Fluid Reservoir. See "Adding Washer Fluid" under Windshield Washer Fluid.

2. Coolant Surge Tank and Pressure Cap. See Cooling System.

3. Brake Master Cylinder Reservoir. See "Brake Fluid" under Brakes and Hydraulic Clutch.

4. Engine Oil Dipstick (Out of View). See "Checking Engine Oil" under Engine Oil.

5. Engine Air Cleaner/Filter.

6. Engine Oil Fill Cap. See "When to Add Engine Oil" under Engine Oil.

7. Power Steering Fluid Reservoir. See Power Steering Fluid.

8. Remote Negative (-) Ground (Out of View). See Jump Starting.

9. Battery (Out of View).

10. Remote Positive (+) Terminal. See Jump Starting.

11. Underhood Fuse Block.

When you open the hood on the 2.0L L4 engine, this is what you will see:

1. Windshield Washer Fluid Reservoir. See "Adding Washer Fluid" under Windshield Washer Fluid.

2. Coolant Surge Tank and Pressure Cap. See Cooling System.

3. Brake Master Cylinder Reservoir. See "Brake Fluid" under Brakes and Hydraulic Clutch.

4. Engine Oil Dipstick. See "Checking Engine Oil" under Engine Oil.

5. Engine Air Cleaner/Filter.

6. Engine Oil Fill Cap. See "When to Add Engine Oil" under Engine Oil.

7. Power Steering Fluid Reservoir. See Power Steering Fluid.

8. Remote Negative (-) Ground (Out of View). See Jump Starting.

9. Battery (Out of View).

10. Remote Positive (+) Terminal. See Jump Starting.

11. Underhood Fuse Block.