For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Air Cleaner Outlet Duct Resonator Clamp Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m (80 lb in)
2 | Air Cleaner Outlet Duct Resonator Clamp Tighten 9 N·m (80 lb in)
3 | Positive Crankcase Ventilation Hose Clamp
4 | Air Cleaner Outlet Duct Resonator Tip Pull up on the outlet duct assembly in order to disengage the assembly from the studs.