For 1990-2009 cars

Callout | Component Name
--- | ---
Caution: Refer to Fastener Caution in the Preface section. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications.

#### Preliminary Procedure

Drain the cooling system. Refer to Cooling System Draining and Filling.

1 | Hose Assembly, Radiator Surge Tank Inlet Tip

• | Using J 38185 position radiator surge tank outlet hose clamps aside and remove hose from the fittings.

• | Note routing of the radiator surge tank inlet hose to ensure proper insulation.