For 1990-2009 cars

## Power Brake Booster Vacuum Check Valve and Hose Replacement J65

Callout | Component Name
--- | ---
1 | Power Brake Booster Vacuum Hose Clamp
2 | Power Brake Booster Vacuum Hose Clamp
3 | Power Brake Booster Vacuum Hose Tip If necessary, a small amount of denatured alcohol can be used as an assembly aid for installing the vacuum hose to the check valve. Do not use soap.
4 | Power Brake Booster Vacuum Check Valve Tip If necessary, a small amount of denatured alcohol can be used as an assembly aid for installing the check valve to the booster grommet. Do not use soap.

## Power Brake Booster Vacuum Check Valve and Hose Replacement JL9

Callout | Component Name
--- | ---

#### Preliminary Procedure

Disconnect the power brake booster vacuum sensor electrical connector.

1 | Power Brake Booster Vacuum Hose Clamp
2 | Power Brake Booster Vacuum Hose Clamp
3 | Power Brake Booster Vacuum Hose Tip If necessary, a small amount of denatured alcohol can be used as an assembly aid for installing the vacuum hose to the check valve. Do not use soap.
4 | Power Brake Booster Vacuum Sensor and Check Valve Tip If necessary, a small amount of denatured alcohol can be used as an assembly aid for installing the check valve to the booster grommet. Do not use soap.