For 1990-2009 cars

Callout | Component Name
--- | ---
Fastener Tightening Specifications: Refer to Fastener Tightening Specifications .

#### Preliminary Procedure

Remove the wiper arms. Refer to Windshield Wiper Arm Replacement .

1 | Air Inlet Grille Retainers (Qty: 10)
2 | Air Inlet Grille
3 | Air Inlet Grille Tape (Qty: 2) Tip Clean the air inlet grille with P/N 12378462 before installing the tape.