For 1990-2009 cars

Figure 1: |

#### Engine Harness Routing Views 1 of 2 (LNF)

(1) | Fuse Block-Underhood
(2) | C162
(3) | Transmission Control Module (TCM) (M82)
(4) | Engine Control Module (ECM) Bracket
(5) | S137
(6) | S142
(8) | S120
(9) | Engine Harness

Figure 2: |

#### Engine Harness Routing Views 2 of 2 (LNF)

(1) | S123
(2) | S124
(3) | Engine Harness
(4) | S121
(5) | C100
(6) | Fuse Block - Underhood
(7) | G103
(8) | S140
(9) | S107
(10) | C101 (M82)
(11) | Automatic Transmission (M82)

Figure 3: |

#### Above the Radiator

(1) | Air Cleaner
(2) | Mass Air Flow (MAF) / Intake Air Temperature (IAT) Sensor

Figure 4: |

#### Left Side of Engine (1 of 2) (LNF)

(1) | Manifold Absolute Pressure (MAP) Sensor
(2) | Throttle Body
(3) | Starter Motor
(4) | A/C Compressor
(5) | Generator
(6) | Evaporative Emission (EVAP) Canister Purge Solenoid Valve

Figure 5: |

#### Left Side of Engine Compartment - LNF

(1) | Fuel Rail Pressure (FRP) Sensor
(2) | Intake Air Pressure and Temperature Sensor
(3) | Brake Booster Vacuum Sensor
(4) | Brake Fluid Level Switch
(5) | Brake Booster Pump Motor

Figure 6: |

#### Right Side of Engine (LNF)

(1) | Turbocharger
(2) | Heated Oxygen Sensor (HO2S) 2
(3) | Heated Oxygen Sensor (HO2S) 1
(4) | Camshaft Position (CMP) Sensor - Exhaust

Figure 7: |

#### Left Side of Engine (LNF)

(1) | Ignition Coil 1
(2) | Ignition Coil 2
(3) | Ignition Coil 3
(4) | Ignition Coil 4
(5) | High Pressure Fuel Pump
(6) | Fuel Injector 1
(7) | Fuel Injector 2
(8) | Fuel Injector 3
(9) | Fuel Injector 4
(10) | Manifold Absolute Pressure (MAP) Sensor
(11) | Engine Oil Pressure (EOP) Switch
(12) | Crankshaft Position (CKP) Sensor
(13) | Knock Sensor (KS) 2
(14) | Starter Motor
(15) | Evaporative Emission (EVAP) Canister Purge Solenoid Valve
(16) | Camshaft Position (CMP) Actuator Solenoid - Exhaust
(17) | Camshaft Position (CMP) Actuator Solenoid - Intake

Figure 8: |

#### Lower Left Side of I/P

(1) | Brake Pedal Position Sensor
(2) | Accelerator Pedal Position (APP) Sensor
(3) | Data Link Connector (DLC)
(4) | Data Link Terminator Resistor
(5) | Clutch Pedal Position (CPP) Switch (MA5)
(6) | Clutch Start Switch (MA5)
(7) | C500
(8) | C501
(9) | Steering Angle Sensor (JL4)