For 1990-2009 cars

Callout | Component Name
--- | ---
Notice: Refer to Fastener Notice in the Preface section. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications.

#### Preliminary Procedure

1. Remove the lower I/P extension panel. Refer to Instrument Panel Extension Trim Plate Replacement.
2. Disconcert the electrical connector for the traction control switch.

1 | Switch, Traction Control. Tip Depress the retaining clip for the traction control switch before removing the switch.