For 1990-2009 cars

## Fastener Tightening Specifications Solstice

Application | Specification
--- | ---
Metric | English
Instrument Panel Assist Handle | 9 N·m | 80 lb in
Instrument Panel Carrier Bolts | 9 N·m | 80 lb in
Instrument Panel Carrier Nuts | 9 N·m | 80 lb in
Instrument Panel Carrier Screws | 2 N·m | 18 lb in
Instrument Panel Closeout/Insulator Panel Screws | 2 N·m | 18 lb in
Instrument Panel Compartment Dampener Screws | 2 N·m | 18 lb in
Instrument Panel Compartment Latch Screws | 2 N·m | 18 lb in
Instrument Panel Compartment Striker Screws | 2 N·m | 18 lb in
Instrument Panel Extension Trim Plate Screws | 2 N·m | 18 lb in
Instrument Panel Tie Bar to Hinge Pillar Bolts | 25 N·m | 18 lb ft
Instrument Panel Tie Bar to Tunnel Bolts | 12 N·m | 106 lb in
Instrument Panel Upper Trim Pad | 2 N·m | 18 lb in
Knee Bolster Bracket Bolts | 9 N·m | 80 lb in
Knee Bolster Panel Screws | 2 N·m | 18 lb in

## Fastener Tightening Specifications SKY

Application | Specification
--- | ---
Metric | English
Instrument Panel Carrier Bolts | 9 N·m | 80 lb in
Instrument Panel Carrier Nuts | 9 N·m | 80 lb in
Instrument Panel Carrier Screws | 9 N·m | 80 lb in
Instrument Panel Center Support Bracket Screw/Bolts | 2 N·m | 18 lb in
Instrument Panel Center Support to Floor Panel Bolt/Screw | 58 N·m | 43 lb ft
Instrument Panel Closeout/Insulator Panel Screws | 2.5 N·m | 22 lb in
Instrument Panel Cluster Trim Bezel Screws | 2.5 N·m | 22 lb in
Instrument Panel Compartment Dampener Screws | 2.5 N·m | 22 lb in
Instrument Panel Compartment Door Opening Frame Screws/Bolts | 2.5 N·m | 22 lb in
Instrument Panel Compartment Latch Screws | 2.5 N·m | 22 lb in
Instrument Panel Lower Trim Panel | 2.5 N·m | 22 lb in
Instrument Panel Tie Bar to Hinge Pillar Bolts | 25 N·m | 18 lb ft
Instrument Panel Tie Bar to Tunnel Bolts | 12 N·m | 106 lb in
Instrument Panel Upper Trim Panel | 2.5 N·m | 22 lb in
Knee Bolster Bracket Bolts | 9 N·m | 80 lb in
Knee Bolster Panel Screws | 2.5 N·m | 22 lb in
Front Floor Lower Console Screws/Bolts | 2.5 N·m | 22 lb in