For 1990-2009 cars

## Instrument Panel Compartment Door Dampener Replacement Sky

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the instrument panel (I/P) compartment. Refer to Instrument Panel Compartment Replacement.

1 | I/P Compartment Dampener Screw (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | I/P Compartment Dampener Assembly

## Instrument Panel Compartment Door Dampener Replacement Solstice

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the instrument panel (I/P) compartment. Refer to Instrument Panel Compartment Replacement.

1 | I/P Compartment Screw (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | I/P Compartment Damper