For 1990-2009 cars

## Digital Radio Antenna Cable Replacement Convertible

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the rear compartment trim. Refer to Rear Compartment Trim Panel Replacement.

1 | Digital Radio Antenna Cable Assembly Tip

1. Disconnect the electrical connectors.
2. Remove the cable conduit, to the rear compartment lid, in order to access the cable connection at the XM radio antenna.