For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front floor console. Refer to Front Floor Console Replacement.

1 | Park Brake Warning Lamp Switch Screw Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (22 lb in)
2 | Park Brake Warning Lamp Switch Tip Disconnect the electrical connector from the park brake warning lamp switch.