For 1990-2009 cars

Connector 1: | C100 Engine Harness to the I/P Body Harness (LNF)
Connector 2: | C100 Engine Harness to the I/P Body Harness (LE5)
Connector 3: | C102 Right Front Fog/Turn Lamp Jumper Harness to the Forward Lamp Harness
Connector 4: | C103 Left Front Fog/Turn Lamp Jumper Harness to the Forward Lamp Harness
Connector 5: | C110 Forward Lamp Harness to Left Headlamp Assembly Harness
Connector 6: | C111 Forward Lamp Harness to Right Headlamp Assembly Harness
Connector 7: | C120 I/P Body Harness to the Forward Lamp Harness
Connector 8: | C160 Engine Harness to the Fuel Injector Jumper Harness (LE5)
Connector 9: | C162 Engine Harness to the Fuel Injector Jumper Harness (LNF)
Connector 10: | C207 I/P Body Harness to the Console Harness (M82)
Connector 11: | C208 Passenger Air Bag Harness to I/P Body Harness
Connector 12: | C216 I/P Body Harness to the HVAC Harness
Connector 13: | C218 I/P Body Harness to the HVAC Harness
Connector 14: | C316 I/P Body Harness to the Passenger Seat Harness
Connector 15: | C317 I/P Body Harness to the Driver Seat Harness (w/o AF2)
Connector 16: | C317 I/P Body Harness to the Driver Seat Harness (AF2)
Connector 17: | C400 I/P Body Harness to the Rear Lamp Harness
Connector 18: | C401 I/P Body Harness to Digital Radio Receiver
Connector 19: | C405 Rear Chassis Harness to Left Tail Lamp Assembly Harness
Connector 20: | C406 I/P Body Harness to Rear Chassis Harness
Connector 21: | C407 Rear Chassis Harness to Right Tail Lamp Assembly Harness
Connector 22: | C408 Rear Chassis Harness to I/P Body Harness
Connector 23: | C500 Driver Door Harness to the I/P Body Harness
Connector 24: | C501 Driver Door Harness to the I/P Body Harness (A31)
Connector 25: | C505 Driver Door Harness to the Power Mirror Harness
Connector 26: | C600 Passenger Door Harness to the I/P Body Harness

### C100 Engine Harness to the I/P Body Harness (LNF)

#### Connector Part Information

- OEM: 15336418
- Service: See Catalog
- Description: 38-Way F GT 150, 280 Series Sealed (BK)

#### Connector Part Information

- OEM: 15317380
- Service: Not Serviced
- Description: 38-Way M GT 150, 280 Series Sealed (BK)

#### Terminal Part Information

- Pins: A1-A3, A8, B1-B3, B5-B6, B8-B12, C1-C7, D1, D6-D7
- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

- Pins: A4, A5, B7
- Terminal/Tray: 15304716/8
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Terminal Part Information

- Pins: A1-A3, A8, B1-B3, B5-B6, B8-B12, C1-C7, D1, D6-D7
- Terminal/Tray: 15326269/19
- Core/Insulation Crimp: E/4
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

- Pins: A4, A5, B7
- Terminal/Tray: 15304728/8
- Core/Insulation Crimp: 2/1
- Release Tool/Test Probe: 15315247/J-35616-5 (PU)

#### C100 Engine Harness to the I/P Body Harness (LNF)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | WH | 1310 | EVAP Canister Vent Solenoid Control | A1 | WH | 1310 | EVAP Canister Vent Solenoid Control
A2 | RD/WH | 840 | Battery Positive Voltage | A2 | RD/WH | 840 | Battery Positive Voltage
A3 | TN | 1274 | 5-Volt Reference 3 | A3 | TN | 1274 | 5-Volt Reference 3
A4 | PU | 92 | Windshield Wiper Motor High Speed | A4 | PU | 92 | Windshield Wiper Motor High Speed
A5 | D-GN | 95 | Windshield Washer Switch Signal | A5 | D-GN | 95 | Windshield Washer Switch Signal
A6-A7 | -- | -- | Not Used | A6-A7 | -- | -- | Not Used
A8 | BN | 4 | Accessory Voltage | A8 | BN | 4 | Accessory Voltage
B1 | BN/WH | 419 | MIL Control | B1 | BN/WH | 419 | MIL Control
B2 | TN/BK | 2500 | High Speed GMLAN Serial Data (+) | B2 | TN/BK | 2500 | High Speed GMLAN Serial Data (+)
B3 | TN | 2501 | High Speed GMLAN Serial Data (-) | B3 | TN | 2501 | High Speed GMLAN Serial Data (-) (1)
B4 | -- | -- | Not Used | B4 | -- | -- | Not Used
B5 | RD/WH | 840 | Battery Positive Voltage (M82) | B5 | RD/WH | 840 | Battery Positive Voltage (M82)
B6 | PU | 1272 | Low Reference | B6 | PU | 1272 | Low Reference
B7 | BK | 250 | Ground | B7 | BK | 250 | Ground
B8 | L-BU | 1162 | APP Sensor 2 Signal | B8 | L-BU | 1162 | APP Sensor 2 Signal
B9 | WH/BK | 1164 | 5-Volt Reference 2 | B9 | WH/BK | 1164 | 5-Volt Reference 2
B10 | BN | 1271 | Low Reference | B10 | BN | 1271 | Low Reference
B11 | D-BU | 1161 | APP Sensor 1 Signal | B11 | D-BU | 1161 | APP Sensor 1 Signal
B12 | TN | 2759 | Low Reference | B12 | TN | 2759 | Low Reference
C1 | PU | 1589 | Fuel Level Sensor Signal | C1 | PU | 1589 | Fuel Level Sensor Signal
C2 | D-GN | 890 | Fuel Tank Pressure Sensor Signal | C2 | D-GN | 890 | Fuel Tank Pressure Sensor Signal
C3 | GY | 2709 | 5-Volt Reference 1 | C3 | GY | 2709 | 5-Volt Reference 1
C4 | D-GN/WH | 465 | Fuel Pump Relay Control | C4 | D-GN/WH | 465 | Fuel Pump Relay Control
C5 | YE | 196 | Windshield Wiper Motor Park Switch Signal | C5 | YE | 196 | Windshield Wiper Motor Park Switch Signal
C6 | PK/BK | 5291 | Ignition 1 Voltage | C6 | PK/BK | 5291 | Ignition 1 Voltage
C7 | PK | 849 | Brake Fluid Level Sensor Signal 20 | C7 | PK | 849 | Brake Fluid Level Sensor Signal
C8-C12 | -- | -- | Not Used | C8-C12 | -- | -- | Not Used
D1 | BN/WH | 379 | CPP Switch Signal (MA5) | D1 | BN/WH | 379 | CPP Switch Signal (MA5)
D2-D3 | -- | -- | Not Used | D2-D3 | -- | -- | Not Used
D4-D5 | -- | -- | Not Available | D4-D5 | -- | -- | Not Available
D6 | L-GN | 1478 | Coolant Level Switch Signal | D6 | L-GN | 1478 | Coolant Level Switch Signal
D7 | OG | 228 | Windshield Washer Pump Control | D7 | OG | 228 | Windshield Washer Pump Control
D8 | -- | -- | Not Used | D8 | -- | -- | Not Used

### C100 Engine Harness to the I/P Body Harness (LE5)

#### Connector Part Information

- OEM: 15443822
- Service: See Catalog
- Description: 38-Way F GT 150, 280 Series Sealed (BK)

#### Connector Part Information

- OEM: 15317380
- Service: Not Serviced
- Description: 38-Way GT 150, 280 Series Sealed (BK)

#### Terminal Part Information

- Pins: A1-A3, A8, B1-B3, B5-B6, B8-B12, C1-C7, D1, D6-D7
- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

- Pins: A4, A5, B7
- Terminal/Tray: 15304716/8
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Terminal Part Information

- Pins: A1-A3, A8, B1-B3, B5-B6, B8-B12, C1-C7, D1, D6-D7
- Terminal/Tray: 15326269/19
- Core/Insulation Crimp: E/4
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

- Pins: A4, A5, B7
- Terminal/Tray: 15304728/8
- Core/Insulation Crimp: 2/1
- Release Tool/Test Probe: 15315247/J-35616-5 (PU)

#### C100 Engine Harness to the I/P Body Harness (LE5)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | WH | 1310 | EVAP Canister Vent Solenoid Control | A1 | WH | 1310 | EVAP Canister Vent Solenoid Control
A2 | RD/WH | 840 | Battery Positive Voltage | A2 | RD/WH | 840 | Battery Positive Voltage
A3 | TN | 1274 | 5-Volt Reference 3 | A3 | TN | 1274 | 5-Volt Reference 3
A4 | PU | 92 | Windshield Wiper Motor High Speed | A4 | PU | 92 | Windshield Wiper Motor High Speed
A5 | D-GN | 95 | Windshield Washer Switch Signal | A5 | D-GN | 95 | Windshield Washer Switch Signal
A6-A7 | -- | -- | Not Used | A6-A7 | -- | -- | Not Used
A8 | BN | 4 | Accessory Voltage | A8 | BN | 4 | Accessory Voltage
B1 | BN/WH | 419 | MIL Control | B1 | BN/WH | 419 | MIL Control
B2 | TN/BK | 2500 | High Speed GMLAN Serial Data (+) | B2 | TN/BK | 2500 | High Speed GMLAN Serial Data (+)
B3 | TN | 2501 | High Speed GMLAN Serial Data (-) | B3 | TN | 2501 | High Speed GMLAN Serial Data (-) (1)
B4 | -- | -- | Not Used | B4 | -- | -- | Not Used
B5 | RD/WH | 840 | Battery Positive Voltage (M82) | B5 | RD/WH | 840 | Battery Positive Voltage (M82)
B6 | PU | 1272 | Low Reference | B6 | PU | 1272 | Low Reference
B7 | BK | 250 | Ground | B7 | BK | 250 | Ground
B8 | L-BU | 1162 | APP Sensor 2 Signal | B8 | L-BU | 1162 | APP Sensor 2 Signal
B9 | WH/BK | 1164 | 5-Volt Reference 2 | B9 | WH/BK | 1164 | 5-Volt Reference 2
B10 | BN | 1271 | Low Reference | B10 | BN | 1271 | Low Reference
B11 | D-BU | 1161 | APP Sensor 1 Signal | B11 | D-BU | 1161 | APP Sensor 1 Signal
B12 | TN | 2759 | Low Reference | B12 | TN | 2759 | Low Reference
C1 | PU | 1589 | Fuel Level Sensor Signal | C1 | PU | 1589 | Fuel Level Sensor Signal
C2 | D-GN | 890 | Fuel Tank Pressure Sensor Signal | C2 | D-GN | 890 | Fuel Tank Pressure Sensor Signal
C3 | GY | 2709 | 5-Volt Reference 1 | C3 | GY | 2709 | 5-Volt Reference 1
C4 | D-GN/WH | 465 | Fuel Pump Relay Control | C4 | D-GN/WH | 465 | Fuel Pump Relay Control
C5 | YE | 196 | Windshield Wiper Motor Park Switch Signal | C5 | YE | 196 | Windshield Wiper Motor Park Switch Signal
C6 | PK/BK | 5291 | Ignition 1 Voltage | C6 | PK/BK | 5291 | Ignition 1 Voltage
C7 | PK | 849 | Brake Fluid Level Sensor Signal | C7 | PK | 849 | Brake Fluid Level Sensor Signal
C8-C12 | -- | -- | Not Used | C8-C12 | -- | -- | Not Used
D1 | BN/WH | 379 | CPP Switch Signal (MA5) | D1 | BN/WH | 379 | CPP Switch Signal (MA5)
D2-D3 | -- | -- | Not Used | D2-D3 | -- | -- | Not Used
D4-D5 | -- | -- | Not Available | D4-D5 | -- | -- | Not Available
D6 | L-GN | 1478 | Coolant Level Switch Signal | D6 | L-GN | 1478 | Coolant Level Switch Signal
D7 | OG | 228 | Windshield Washer Pump Control | D7 | OG | 228 | Windshield Washer Pump Control
D8 | -- | -- | Not Used | D8 | -- | -- | Not Used

### C102 Right Front Fog/Turn Lamp Jumper Harness to the Forward Lamp Harness

#### Connector Part Information

- OEM: 12186568
- Service: See Catalog
- Description: 4-Way F Metri-Pack 150 Series Sealed (BK)

#### Connector Part Information

- OEM: 12186271
- Service: 15306054
- Description: 4-Way M Metri-Pack 150 Series Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: 12047553/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-3 (GY)

#### Terminal Part Information

- Terminal/Tray: 12045773/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-3 (GY)

#### C102 Right Front Fog/Turn Lamp Jumper Harness to the Forward Lamp Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | D-BU | 15 | Right Turn Signal Lamp Supply Voltage | A | D-BU | 15 | Right Turn Signal Lamp Supply Voltage
B | BN | 9 | Park Lamp Supply Voltage | B | BN | 9 | Park Lamp Supply Voltage
C | PU | 2234 | Front Fog Lamp Supply Voltage (T96) | C | PU | 2234 | Front Fog Lamp Supply Voltage (T96)
D | BK | 250 | Ground | D | BK | 250 | Ground

### C103 Left Front Fog/Turn Lamp Jumper Harness to the Forward Lamp Harness

#### Connector Part Information

- OEM: 12186568
- Service: See Catalog
- Description: 4-Way F Metri-Pack 150 Series Sealed (BK)

#### Connector Part Information

- OEM: 12186271
- Service: 15306054
- Description: 4-Way M Metri-Pack 150 Series Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: 12047553/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-3 (GY)

#### Terminal Part Information

- Terminal/Tray: 12045773/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-3 (GY)

#### C103 Left Front Fog/Turn Lamp Jumper Harness to the Forward Lamp Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | L-BU | 14 | Left Turn Signal Lamp Supply Voltage | A | L-BU | 14 | Left Turn Signal Lamp Supply Voltage
B | BN | 9 | Park Lamp Feed | B | BN | 9 | Park Lamp Feed
C | PU | 2234 | Front Fog Lamp Supply Voltage (T96) | C | PU | 2234 | Front Fog Lamp Supply Voltage (T96)
D | BK | 150 | Ground | D | BK | 150 | Ground

### C110 Forward Lamp Harness to Left Headlamp Assembly Harness

#### Connector Part Information

- OEM: 15326815
- Service: 15306396
- Description: 4-Way F GT 150 Series, Sealed (BK)

#### Connector Part Information

- OEM: 15369319
- Service: See Catalog
- Description: 4-Way M GT 150 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C110 Forward Lamp Harness to Left Headlamp Assembly Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | D-GN/WH | 711 | Left Headlamp High Beam Supply Voltage | A | BK | -- | Left Headlamp High Beam Supply Voltage
B | BK | 150 | Ground | B | BK | -- | Ground
C | YE | 712 | Left Headlamp Low Beam Supply Voltage | C | RD | -- | Left Headlamp Low Beam Supply Voltage
D | BK | 150 | Ground | D | RD | -- | Ground

### C111 Forward Lamp Harness to Right Headlamp Assembly Harness

#### Connector Part Information

- OEM: 15326815
- Service: 15306396
- Description: 4-Way F GT 150 Series, Sealed (BK)

#### Connector Part Information

- OEM: 15369319
- Service: See Catalog
- Description: 4-Way M GT 150 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C111 Forward Lamp Harness to Right Headlamp Assembly Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | L-GN/BK | 311 | Right Headlamp High Beam Supply Voltage | A | BK | -- | Right Headlamp High Beam Supply Voltage
B | BK | 250 | Ground | B | BK | -- | Ground
C | TN/WH | 312 | Right Headlamp Low Beam Supply Voltage | C | RD | -- | Right Headlamp Low Beam Supply Voltage
D | BK | 250 | Ground | D | RD | -- | Ground

### C120 I/P Body Harness to the Forward Lamp Harness

#### Connector Part Information

- OEM: 15326084
- Service: 15306348
- Description: 16-Way F GT 150 280 Series Sealed 4.0 5.8 (BK)

#### Connector Part Information

- OEM: 15326085
- Service: 15306122
- Description: 16-Way M GT 150 280 Series Sealed 4.0 5.8 (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C120 I/P Body Harness to the Forward Lamp Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | PK/BK | 6434 | Can Bus High Serial Data (JL4) | A | PK/BK | 6434 | Can Bus High Serial Data (JL4)
B | TN | 884 | Left Rear Wheel Speed Sensor Signal (JL9) | B | TN | 884 | Left Rear Wheel Speed Sensor Signal (JL9)
C | OG | 885 | Left Rear Wheel Speed Sensor Low Reference (JL9) | C | OG | 885 | Left Rear Wheel Speed Sensor Low Reference (JL9)
D | BN | 882 | Right Rear Wheel Speed Sensor Signal (JL9) | D | BN | 882 | Right Rear Wheel Speed Sensor Signal (JL9)
E | WH | 883 | Right Rear Wheel Speed Sensor Low Reference (JL9) | E | WH | 883 | Right Rear Wheel Speed Sensor Low Reference (JL9)
F | TN/BK | 2500 | High Speed GMLAN Serial Data (+) | F | TN/BK | 2500 | High Speed GMLAN Serial Data (+) (1) (JL9)
F | TN/BK | 2500 | High Speed GMLAN Serial Data (+) (UE1) | F | TN/BK | 2500 | High Speed GMLAN Serial Data (+)
G | TN | 2501 | High Speed GMLAN Serial Data (-) | G | TN | 2501 | High Speed GMLAN Serial Data (-) (JL9)
G | TN | 2501 | High Speed GMLAN Serial Data (-) (1) (UE1) | G | TN | 2501 | High Speed GMLAN Serial Data (-) (1)
H | D-GN | 2087 | 12-Volt Reference (JL4) | H | D-GN | 2087 | 12-Volt Reference (JL4)
J | L-BU | 2088 | Low Reference (JL4) | J | L-BU | 2088 | Low Reference (JL4)
K | TN/BK | 2500 | High Speed GMLAN Serial Data (+) | K | TN/BK | 2500 | High Speed GMLAN Serial Data (+) (JL9)
K | TN/BK | 2500 | High Speed GMLAN Serial Data (+)
L | TN | 2501 | High Speed GMLAN Serial Data (-) | L | TN | 2501 | High Speed GMLAN Serial Data (-) (1) (JL9)
L | TN | 2501 | High Speed GMLAN Serial Data (-)
M | YE/BK | 2160 | Front End Discriminating Sensor Signal | M | YE/BK | 2160 | Front End Discriminating Sensor Signal
N | GY | 5600 | Right Front Discriminating Sensor Low Reference | N | GY | 5600 | Right Front Discriminating Sensor Low Reference
P | YE | 1834 | Forward Discriminating Sensor Signal | P | YE | 1834 | Forward Discriminating Sensor Signal
R | TN/OG | 5045 | Left Front Discriminating Sensor Low Reference | R | TN/OG | TN/OG | Left Front Discriminating Sensor Low Reference
S | GY/BK | 6435 | CAN Bus Low Serial Data (JL4) | S | GY/BK | 6435 | CAN Bus Low Serial Data (JL4)

### C160 Engine Harness to the Fuel Injector Jumper Harness (LE5)

#### Connector Part Information

- OEM: 15326835
- Service: 88986452
- Description: 8-Way F GT 150 Series Sealed 4.0 (BK)

#### Connector Part Information

- OEM: 15326840
- Service: See Catalog
- Description: 8-Way M GT 150 Series Sealed 4.0 (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C160 Engine Harness to the Fuel Injector Jumper Harness (LE5)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BK | 1744 | Fuel Injector 1 Control | A | BK | 1744 | Fuel Injector 1 Control
B | L-GN/BK | 1745 | Fuel Injector 2 Control | B | L-GN/BK | 1745 | Fuel Injector 2 Control
C | PK/BK | 1746 | Fuel Injector 3 Control | C | PK/BK | 1746 | Fuel Injector 3 Control
D | L-BU/BK | 844 | Fuel Injector 4 Control | D | BU/BK | 844 | Fuel Injector 4 Control
E | PK/BK | 5292 | Ignition 1 Voltage | E | PK | 139 | Ignition 1 Voltage
F | OG/BK | 469 | Low Reference | F | OG/BK | 469 | Low Reference
G | L-GN | 432 | MAP Sensor Signal | G | L-GN | 432 | MAP Sensor Signal
H | GY | 2704 | 5-Volt Reference | H | GY | 2704 | 5-Volt Reference

### C162 Engine Harness to the Fuel Injector Jumper Harness (LNF)

#### Connector Part Information

- OEM: 33472-1216
- Service: See Catalog
- Description: 12-Way F

#### Connector Part Information

- OEM: 33482-1206
- Service: See Catalog
- Description: 12-Way M

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C162 Engine Harness to the Fuel Injector Jumper Harness (LNF)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | BN | 4801 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 1 | 1 | BN | 4801 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 1
2 | D-BU | 4802 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 2 | 2 | BN | 4802 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 2
3 | D-GN | 4803 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 3 | 3 | BN | 4803 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 3
4 | L-BU | 4804 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 4 | 4 | BN | 4804 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 4
5 | TN | 808 | Low Reference | 5 | GN | 808 | Low Reference
6 | -- | -- | Not Used | 6 | -- | -- | Not Used
7 | BN/WH | 4901 | Direct Fuel Injector (DFI) High Voltage Supply Cylinder 1 | 7 | BN | 4901 | Direct Fuel Injector (DFI) High Voltage Supply Cylinder 1
8 | D-BU/Wh | 4902 | Direct Fuel Injector (DFI) High Voltage Supply Cylinder 2 | 8 | BN | 4902 | Direct Fuel Injector (DFI) High Voltage Supply Cylinder 2
9 | D-GN/WH | 4903 | Direct Fuel Injector (DFI) High Voltage Supply Cylinder 3 | 9 | BN | 4903 | Direct Fuel Injector (DFI) High Voltage Supply Cylinder 3
10 | L-BU/WH | 4904 | Direct Fuel Injector (DFI) High Voltage Supply Cylinder 4 | 10 | BN | 4904 | Direct Fuel Injector (DFI) High Voltage Supply Cylinder 4
11 | GY | 598 | 5-Volt Reference | 11 | GN | 598 | 5-Volt Reference
12 | YE | 2918 | FRP Sensor Signal | 12 | GN | 2918 | FRP Sensor Signal

### C207 I/P Body Harness to the Console Harness (M82)

#### Connector Part Information

- OEM: E-3581-001
- Service: See Catalog
- Description: 12-Way F 1.5 Series (NA)

#### Connector Part Information

- OEM: E-3584-003
- Service: 88988763
- Description: 12-Way M 1.5 Series (NA)

#### Terminal Part Information

- Terminal/Tray: 7116-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: 7114-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### C207 I/P Body Harness to the Console Harness (M82)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | L-GN/WH | 5984 | PRNDL Signal D | 1 | L-GN/WH | 5984 | PRNDL Signal D
2 | OG/BK | 5983 | PRNDL Signal C | 2 | OG/BK | 5983 | PRNDL Signal C
3 | PK/BK | 5982 | PRNDL Signal B | 3 | PK/BK | 5982 | PRNDL Signal B
4 | PU/WH | 5981 | PRNDL Signal A | 4 | PU/WH | 5981 | PRNDL Signal A
5 | GY | 8 | Instrument Panel Lamp Supply Voltage | 5 | GY | 8 | Instrument Panel Lamp Supply Voltage
6 | BN | 4 | Accessory Voltage | 6 | BN | 4 | Accessory Voltage
7 | D-GN/WH | 1135 | A/T Shift Lock Control Solenoid Supply Voltage | 7 | D-GN/WH | 1135 | A/T Shift Lock Control Solenoid Supply Voltage
8 | BK/WH | 651 | Ground | 8 | BK/WH | 651 | Ground
9 | BN | 550 | Ground | 9 | BK | 550 | Ground
10 | BU | 1932 | Ignition Lock Cylinder Control Actuator Signal | 10 | D-GN/WH | 1932 | Ignition Lock Cylinder Control Actuator Signal
11-12 | -- | -- | Not Used | 11-12 | -- | -- | Not Used

### C208 Passenger Air Bag Harness to I/P Body Harness

#### Connector Part Information

- OEM: 15336479
- Service: 88988600
- Description: 4-Way F Metri-Pack 280 (YE)

#### Connector Part Information

- OEM: 15336476
- Service: 15306363
- Description: 4-Way M Metri-Pack 280 Series (YE)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: 12034047/2
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

#### C208 Passenger Air Bag Harness to I/P Body Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | OG | 3024 | I/P Module - Stage 1 - Low Control | A1 | OG | 3024 | I/P Module - Stage 1 - Low Control
A2 | YE | 3025 | I/P Module - Stage 1 - High Control | A2 | YE | 3025 | I/P Module - Stage 1 - High Control
B1 | PU | 3026 | I/P Module - Stage 2 - Low Control | B1 | PU | 3026 | I/P Module - Stage 2 - Low Control
B2 | GY | 3027 | I/P Module - Stage 2 - High Control | B2 | GY | 3027 | I/P Module - Stage 2 - High Control

### C216 I/P Body Harness to the HVAC Harness

#### Connector Part Information

- OEM: 6098-4787
- Service: See Catalog
- Description: 8-Way F (NA)

#### Connector Part Information

- OEM: 6098-4905
- Service: See Catalog
- Description: 8-Way M 2.8 mm Conn (NA)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C216 I/P Body Harness to the HVAC Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | YE | 60 | Blower Motor Low Control | 1 | YE | 60 | Blower Motor Low Control
2 | TN | 63 | Blower Motor Medium 1 Control | 2 | TN | 63 | Blower Motor Medium 1 Control
3 | L-BU | 72 | Medium 2 Blower Motor Control | 3 | L-BU | 72 | Medium 2 Blower Motor Control
4 | OG | 52 | Blower Motor High Control | 4 | OG | 52 | Blower Motor High Control
5 | BN | 141 | Ignition 3 Voltage | 5 | BN | 141 | Ignition 3 Voltage
6 | BK | 2050 | Ground | 6 | BK | 550 | Ground
7-8 | -- | -- | Not Used | 7-8 | -- | -- | Not Used

### C218 I/P Body Harness to the HVAC Harness

#### Connector Part Information

- OEM: 6098-4789
- Service: See Catalog
- Description: 12-Way F (NA)

#### Connector Part Information

- OEM: 6098-4900
- Service: See Catalog
- Description: 12-Way M (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C218 I/P Body Harness to the HVAC Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | TN/BK | 2274 | Recirculation Door Control Circuit | 1 | L-GN | 2274 | Recirculation Door Control Circuit
2 | D-GN | 1614 | Recirculation Door Control | 2 | L-BU | 1614 | Recirculation Door Control
3 | D-BU | 1646 | Auxiliary Air Temperature Door Position Signal | 3 | D-BU | 1646 | Auxiliary Air Temperature Door Position Signal
4 | L-GN | 2275 | Mode Door Position Signal | 4 | L-GN | 2275 | Mode Door Position Signal
5 | L-GN/BK | 1647 | Recirculation Door Control B | 5 | L-GN/BK | 1647 | Recirculation Door Control B
6 | L-BU/BK | 1688 | 5-Volt Reference | 6 | L-BU/BK | 1688 | 5-Volt Reference
7 | L-GN/BK | 2276 | Defrost Door Position Signal | 7 | L-GN/BK | 2276 | Defrost Door Position Signal
8 | TN | 2273 | Mode Door Control | 8 | TN | 2273 | Mode Door Control
9 | D-BU | 1199 | Air Temperature Door Control | 9 | D-BU | 1199 | Air Temperature Door Control
10 | L-BU | 733 | Air Temperature Door Position Signal | 10 | L-BU | 733 | Air Temperature Door Position Signal
11 | GY | 6137 | EVAP Core Temperature Sensor Signal (C60) | 11 | GY | 6137 | EVAP Core Temperature Sensor Signal (C60)
12 | YE | 1791 | Low Reference | 12 | YE | 1791 | Low Reference

### C316 I/P Body Harness to the Passenger Seat Harness

#### Connector Part Information

- OEM: 15332145
- Service: 15306407
- Description: 8-Way F GT 150 Series (BK)

#### Connector Part Information

- OEM: 15332150
- Service: 88986250
- Description: 8-Way M GT 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C316 I/P Body Harness to the Passenger Seat Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | OG | 1362 | Seat Belt Switch - Right - Signal | A | OG | 1362 | Seat Belt Switch - Right - Signal
B | -- | -- | Not Used | B | -- | -- | Not Used
C | PK | 5057 | Seat Position Sensor - Low Reference | C | PK | 5057 | Seat Position Sensor - Low Reference
D | PK | 353 | I/P Module Suppression Indicator Control | D | PK | 353 | I/P Module Suppression Indicator Control
E | TN/BK | 723 | I/P Module Disable Switch - Signal | E | TN/BK | 723 | I/P Module Disable Switch - Signal
F | PK | 1339 | Ignition 1 Voltage | F | PK | 1339 | Ignition 1 Voltage
G | PK | 5018 | Occupant Sensor Serial Data | G | PK | 5018 | Occupant Sensor Serial Data
H | BK/WH | 351 | Ground | H | BK/WH | 351 | Ground

### C317 I/P Body Harness to the Driver Seat Harness (w/o AF2)

#### Connector Part Information

- OEM: 15332132
- Service: 88953364
- Description: 3-Way F GT 150 Series (BK)

#### Connector Part Information

- OEM: 15332133
- Service: 88987881
- Description: 3-Way M GT 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C317 I/P Body Harness to the Driver Seat Harness (w/o AF2)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | TN/WH | 238 | Seat Belt Switch Signal | A | TN/WH | 238 | Seat Belt Switch Signal
B | -- | -- | Not Used | B | -- | -- | Not Used
C | PK | 5057 | Seat Position Sensor - Low Reference | C | PK | 5057 | Seat Position Sensor - Low Reference

### C317 I/P Body Harness to the Driver Seat Harness (AF2)

#### Connector Part Information

- OEM: 15326886
- Service: See Catalog
- Description: 4-Way F GT 280 (BK)

#### Connector Part Information

- OEM: 15326890
- Service: See Catalog
- Description: 4-Way M GT 280 (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C317 I/P Body Harness to the Driver Seat Harness (AF2)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | TN/WH | 238 | Driver Seat Belt Switch Signal | A | TN/WH | 238 | Driver Seat Belt Switch Signal
B | PK | 5057 | Seat Position Switch Low Reference | B | PK | 5057 | Seat Position Switch Low Reference
C | RD/BK | 642 | Battery Positive Voltage | C | PK | 5057 | Battery Positive Voltage
D | BK | 550 | Ground | D | BK | 550 | Ground

### C400 I/P Body Harness to the Rear Lamp Harness

#### Connector Part Information

- OEM: E-3166-000
- Service: 88988062
- Description: 4-Way F (BK)

#### Connector Part Information

- OEM: E-5345-002
- Service: 88988064
- Description: 4-Way M 1.5 Series (BK)

#### Terminal Part Information

- Pins: 1, 3
- Terminal/Tray: 7116-4103-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

- Pins: 2, 4
- Terminal/Tray: 7116-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Terminal Part Information

- Pins: 1
- Terminal/Tray: 7114-4103-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-3 (GY)

- Pins: 2, 3, 4
- Terminal/Tray: 7114-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-3 (GY)

#### C400 I/P Body Harness to the Rear Lamp Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | BK | 750 | Ground | 1 | BK | 750 | Ground
2 | BN | 9 | Tail/License Park Lamps Supply Voltage | 2 | BN | 9 | Tail/License Park Lamps Supply Voltage
3 | L-GN | 24 | Backup Lamp Supply Voltage | 3 | L-GN | 24 | Backup Lamp Supply Voltage
4 | L-BU | 20 | Stop Lamp Supply Voltage | 4 | L-BU | 20 | Stop Lamp Supply Voltage

### C401 I/P Body Harness to Digital Radio Receiver

#### Connector Part Information

- OEM: 15326924
- Service: See Catalog
- Description: 8-Way F GT 280 Series (BK)

#### Connector Part Information

- OEM: 15326928
- Service: 88988064
- Description: 8-Way M GT 280 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C401 I/P Body Harness to Digital Radio Receiver

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BN/WH | 0367 | Left Audio Signal (+) (UQ3) | A | BN/WH | 367 | Left Audio Signal (+)
B | D-GN/WH | 0368 | Right Audio Signal (+) (UQ3) | B | D-GN/WH | 368 | Right Audio Signal (+)
C | D-GN | 5060 | Low Speed GM LAN Serial Data | C | D-GN | 5060 | Low Speed GM LAN Serial Data
D | BK/WH | 0551 | Ground | D | BK/WH | 551 | Ground
E | TN/WH | 0372 | Audio Common (UQ3) | E | TN/WH | 372 | Audio Common
F | BK | 0814 | Drain Wire | F | BK | 814 | Drain Wire
G | RD/WH | 1340 | Battery Positive Voltage | G | RD/WH | 1340 | Battery Positive Voltage
H | -- | -- | Not Used | H | -- | -- | Not Used

### C405 Rear Chassis Harness to Left Tail Lamp Assembly Harness

#### Connector Part Information

- OEM: 6189-0319
- Service: 88988448
- Description: 6-Way F TS 090 Series Sealed (GY)

#### Connector Part Information

- OEM: 6188-0173
- Service: See Catalog
- Description: 6-Way M TS 090 Series Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: 8100-0461/6
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C405 Rear Chassis Harness to Left Tail Lamp Assembly Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1-2 | -- | -- | Not Used | 1-2 | -- | -- | Not Used
3 | BN | 9 | Tail/License Lamps Supply Voltage | 3 | RD/BU | -- | Tail/License Lamps Supply Voltage
4 | -- | -- | Not Used | 4 | -- | -- | Not Used
5 | BK | 1050 | Ground | 5 | BK | -- | Ground
6 | YE | 18 | Left Rear Stop/Turn Lamp Supply Voltage | 6 | GN | -- | Left Rear Stop/Turn Lamp Supply Voltage

### C406 I/P Body Harness to Rear Chassis Harness

#### Connector Part Information

- OEM: E-5225-001
- Service: 88988066
- Description: 8-Way F Series Sealed (BK)

#### Connector Part Information

- OEM: E-5222-003
- Service: 88988067
- Description: 8-Way M (BK)

#### Terminal Part Information

- Pins: 1-3, 6-8
- Terminal/Tray: 7116-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

- Pins: 4
- Terminal/Tray: 7116-4103-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Terminal Part Information

- Pins: 1-3, 6-8
- Terminal/Tray: 7114-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-3 (GY)

- Pins: 4
- 7114-4103-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-3 (GY)

#### C406 I/P Body Harness to Rear Chassis Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | RD/WH | 140 | Battery Positive Voltage | 1 | RD/WH | 140 | Battery Positive Voltage
2 | WH | 1310 | EVAP Canister Vent Solenoid Control | 2 | WH | 1310 | EVAP Canister Vent Solenoid Control
3 | PU | 1589 | Fuel Level Sensor Signal | 3 | PU | 1589 | Fuel Level Sensor Signal
4 | GY | 120 | Fuel Pump Supply Voltage | 4 | GY | 120 | Fuel Pump Supply Voltage
5 | -- | -- | Not Used | 5 | -- | -- | Not Used
6 | TN | 2759 | Low Reference | 6 | TN | 2759 | Low Reference
7 | D-GN | 890 | Fuel Tank Pressure Sensor Signal | 7 | D-GN | 890 | Fuel Tank Pressure Sensor Signal
8 | GY | 2709 | 5-Volt Reference 1 | 8 | GY | 2709 | 5-Volt Reference 1

### C407 Rear Chassis Harness to Right Tail Lamp Assembly Harness

#### Connector Part Information

- OEM: 6189-0319
- Service: 88988448
- Description: 6-Way F TS 090 Series Sealed (GY)

#### Connector Part Information

- OEM: 6188-0173
- Service: See Catalog
- Description: 6-Way M TS 090 Series Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: 8100-0461/6
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C407 Rear Chassis Harness to Right Tail Lamp Assembly Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1-2 | -- | -- | Not Used | 1-2 | -- | -- | Not Used
3 | BN | 9 | Tail/License Lamps Supply Voltage | 3 | RD/BU | -- | Tail/License Lamps Supply Voltage
4 | -- | -- | Not Used | 4 | -- | -- | Not Used
5 | BK | 750 | Ground | 5 | BK | -- | Ground
6 | D-GN | 19 | Right Rear Stop/Turn Lamp Supply Voltage | 6 | GN | -- | Right Rear Stop/Turn Lamp Supply Voltage

### C408 Rear Chassis Harness to I/P Body Harness

#### Connector Part Information

- OEM: E-5225-001
- Service: 88988066
- Description: 8-Way F Series Sealed (BK)

#### Connector Part Information

- OEM: E-5222-003
- Service: 88988067
- Description: 8-Way M (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4103-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: 7114-4103-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-3 (GY)

#### C408 Rear Chassis Harness to I/P Body Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | BK | 750 | Ground | 1 | BK | 750 | Ground
2 | TN | 884 | Left Rear Wheel Speed Sensor Signal (JL9) | 2 | TN | 884 | Left Rear Wheel Speed Sensor Signal (JL9)
3 | OG | 885 | Left Rear Wheel Speed Sensor Low Reference (JL9) | 3 | OG | 885 | Left Rear Wheel Speed Sensor Low Reference (JL9)
4 | BN | 882 | Right Rear Wheel Speed Sensor Signal (JL9) | 4 | BN | 882 | Right Rear Wheel Speed Sensor Signal (JL9)
5 | WH | 883 | Right Rear Wheel Speed Sensor Low Reference (JL9) | 5 | WH | 883 | Right Rear Wheel Speed Sensor Low Reference (JL9)
6 | YE | 18 | Left Rear Stop/Turn Lamp Supply Voltage | 6 | YE | 18 | Left Rear Stop/Turn Lamp Supply Voltage
7 | BN | 9 | Tail/License Lamps Supply Voltage | 7 | BN | 9 | Tail/License Lamps Supply Voltage
8 | D-GN | 19 | Right Rear Stop/Turn Lamp Supply Voltage | 8 | D-GN | 19 | Right Rear Stop/Turn Lamp Supply Voltage

### C500 Driver Door Harness to the I/P Body Harness

#### Connector Part Information

- OEM: 15326842
- Service: 15326842
- Description: 10-Way F GT 150 Series Sealed (BK)

#### Connector Part Information

- OEM: 15326847
- Service: See Catalog
- Description: 10-Way M GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C500 Driver Door Harness to the I/P Body Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | GY | 118 | Left Front Speaker Output (-) (UW5) | A | GY | 118 | Left Front Speaker Output (-) (UW5)
GY | 118 | Left Front Speaker Output (-) (UQ3) | GY | 118 | Left Front Speaker Output (-) (UQ3)
B | TN | 201 | Left Front Speaker Output (+) (UW5) | B | TN | 201 | Left Front Speaker Output (+) (UW5)
TN | 201 | Left Front Speaker Output (+) (UQ3) | TN | 201 | Left Front Speaker Output (+) (UQ3)
C | GY | 295 | Door Lock Actuator Lock Control (A31) | C | GY | 295 | Door Lock Actuator Lock Control (A31)
D | TN | 694 | Driver Door Lock Actuator Unlock Control (A31) | D | TN | 694 | Driver Door Lock Actuator Unlock Control (A31)
E | GY | 8 | Instrument Panel Lamp Supply Voltage (A31) | E | GY | 8 | Instrument Panel Lamp Supply Voltage (A31)
F | OG/WH | 881 | Passenger Mirror Motor Left Control | F | GY | 881 | Passenger Mirror Motor Left Control
G | PU/WH | 889 | Passenger Mirror Motor Left Control | G | BN/WH | 889 | Passenger Mirror Motor Left Control
H | TN/WH | 330 | Right Mirror Motor Supply Voltage | H | TN/WH | 330 | Right Mirror Motor Supply Voltage
J | RD/WH | 440 | Battery Positive Voltage (A31) | J | RD/WH | 440 | Battery Positive Voltage (A31)
K | GY/BK | 745 | Left Front Door Ajar Switch Signal | K | GY/BK | 745 | Left Front Door Ajar Switch Signal

### C501 Driver Door Harness to the I/P Body Harness (A31)

#### Connector Part Information

- OEM: 15326654
- Service: 88986254
- Description: 8-Way F GT 280 Series Sealed 5.8 (BK)

#### Connector Part Information

- OEM: 15326655
- Service: 15306424
- Description: 8-Way M GT 280 Series Sealed 5.8 (BK)

#### Terminal Part Information

- Terminal: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C501 Driver Door Harness to the I/P Body Harness (A31)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | L-BU | 166 | Power Window Master Switch Right Front Up Signal (A31) | A | L-BU | 166 | Power Window Master Switch Right Front Up Signal (A31)
B | BK | 550 | Ground (A31) | B | BK | 550 | Ground (A31)
C | D-GN | 801 | Retained Accessory Power Fuse Supply Voltage | C | D-GN | 801 | Retained Accessory Power Fuse Supply Voltage
D | TN | 167 | Power Window Master Switch Right Front Down Signal (A31) | D | TN | 167 | Power Window Master Switch Right Front Down Signal (A31)
E | -- | -- | Not Used | E | -- | -- | Not Used
F | WH | 682 | Battery Positive Voltage | F | WH | 682 | Battery Positive Voltage
G-H | -- | -- | Not Used | G-H | -- | -- | Not Used

### C505 Driver Door Harness to the Power Mirror Harness

#### Connector Part Information

- OEM: 15332153
- Service: 88986440
- Description: 10-Way F GT 150 (BK)

#### Connector Part Information

- OEM: 15332158
- Service: 88953270
- Description: 10-Way M GT 150 (BK)

#### Terminal Part Information

- Terminal/Tray:See Terminal Repair Kit
- Core/Insulation Crimp:See Terminal Repair Kit
- Release Tool/Test Probe:See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray:See Terminal Repair Kit
- Core/Insulation Crimp:See Terminal Repair Kit
- Release Tool/Test Probe:See Terminal Repair Kit

#### C505 Driver Door Harness to the Power Mirror Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | -- | -- | Not Used | A | -- | -- | Not Used
B | BK | 550 | Ground | B | BK | 550 | Ground
C | TN/WH | 330 | Passenger Mirror Motor Supply Control | C | TN/WH | 330 | Passenger Mirror Motor Supply Control
D | WH | 81 | Driver Mirror Motor Left Control | D | TN | 81 | Driver Mirror Motor Left Control
E | GY | 8 | Instrument Panel Lamp Supply Voltage | E | GY | 8 | Instrument Panel Lamp Supply Voltage
F | L-GN | 89 | Driver Mirror Motor Up Control | F | L-GN | 89 | Driver Mirror Motor Up Control
G | RD/WH | 440 | Battery Positive Voltage | G | RD/WH | 440 | Battery Positive Voltage
H | TN | 329 | Driver Mirror Motor Supply Voltage | H | TN | 329 | Driver Mirror Motor Supply Voltage
J | OG/WH | 881 | Passenger Mirror Motor Left Control | J | OG/WH | 881 | Passenger Mirror Motor Left Control
K | PU/WH | 889 | Passenger Mirror Motor Up Control | K | PU/WH | 889 | Passenger Mirror Motor Up Control

### C600 Passenger Door Harness to the I/P Body Harness

#### Connector Part Information

- OEM: 15326084
- Service: 15306348
- Description: 16-Way F GT 150 280 Series Sealed 4.0 5.8 (BK)

#### Connector Part Information

- OEM: 15326085
- Service: 15306122
- Description: 16-Way M GT 150 280 Series Sealed 4.0 5.8 (BK)

#### Terminal Part Information

- Terminal: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C600 Passenger Door Harness to the I/P Body Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | L-BU | 166 | Power Window Master Switch Right Front Up Signal (A31) | A | L-BU | 166 | Power Window Master Switch Right Front Up Signal (A31)
B | D-GN | 117 | Right Front Speaker Output (-) | B | D-GN | 117 | Right Front Speaker Output (-)
C | L-GN | 200 | Right Front Speaker Output (+) | C | L-GN | 200 | Right Front Speaker Output (+)
D | TN | 294 | Door Lock Actuator Unlock Control (A31) | D | TN | 294 | Door Lock Actuator Unlock Control (A31)
E | GY | 295 | Door Lock Actuator Lock Control (A31) | E | GY | 295 | Door Lock Actuator Lock Control (A31)
F | GY | 8 | Instrument Panel Lamp Supply Voltage (A31) | F | GY | 8 | Instrument Panel Lamp Supply Voltage (A31)
G | OG/WH | 90 | Passenger Mirror Motor Left Control (A31) | G | GY | 90 | Passenger Mirror Motor Left Control (A31)
H | -- | -- | Not Used | H | -- | -- | Not Used
J | D-GN | 801 | Retained Accessory Power Fuse Supply Voltage | J | D-GN | 801 | Retained Accessory Power Fuse Supply Voltage
K | PK/WH | 889 | Power Mirror Motor RIght Down Control (A31) | K | BN/WH | 1498 | Power Mirror Motor RIght Down Control (A31)
L | TN/WH | 330 | Passenger Mirror Motor Supply Voltage (A31) | L | TN/WH | 330 | Passenger Mirror Motor Supply Voltage (A31)
M | TN/WH | 682 | Battery Positive Voltage | M | TN/WH | 682 | Battery Positive Voltage
N | TN/WH | 746 | Right Front Door Ajar Switch Signal | N | TN/WH | 746 | Right Front Door Ajar Switch Signal (Early)
PK/WH | 746 | Right Front Door Ajar Switch Signal (Late)
P | BK | 550 | Ground (A31) | P | BK | 550 | Ground
R | -- | -- | Not Used | R | -- | -- | Not Used
S | TN | 167 | Power Window Master Switch Right Front Down Signal (A31) | S | TN | 167 | Power Window Master Switch Right Front Down Signal (A31)