For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Catalytic Converter Bracket Bolt/Nut (LNF) | 58 N·m | 43 lb ft
Catalytic Converter to Catalytic Converter Brace Bracket Bolt (LE5) | 50 N·m | 37 lb ft
Catalytic Converter to Catalytic Converter Brace Bracket Bolt (LNF) | 22 N·m | 16 lb ft
Catalytic Converter to Exhaust Manifold Nut (LE5) | 50 N·m | 37 lb ft
Catalytic Converter to Muffler Nut | 17 N·m | 13 lb ft
Catalytic Converter to Turbocharger Nut (LNF) | 58 N·m | 43 lb ft
Engine Mount to Frame Lower Nut (LNF) | 55 N·m | 41 lb ft
Exhaust Manifold Heat Shield Bolt (LNF) | 25 N·m | 18 lb ft
Exhaust Manifold Heat Shield Bolt (LE5) | 10 N·m | 89 lb in
Exhaust Manifold Nut | 14 N·m | 10 lb ft
Turbocharger Heat Shield (LNF) | 10 N·m | 89 lb in