For 1990-2009 cars

Callout | Component Name
--- | ---
Notice: Refer to Fastener Notice in the Preface section. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications .

#### Preliminary Procedures

Open and support the folding top.

1 | Screws, Bow Folding Top No. 3 (Qty: 4) Tighten 10 N·m (89 lb in)
2 | Bow, Folding Top No. 3 Tip It will be necessary to transfer the support strip.