For 1990-2009 cars

## Rear License Plate Lamp Replacement SKY

Callout | Component Name
--- | ---
1 | Rear License Plate Lamp Assembly Screw (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten 2 N·m (18 lb in)
2 | Rear License Plate Lamp Assembly Tip Push one side of the lamp assembly inside the rear bumper cover hole and pull downward to disconnect the electrical connector.
3 | Rear License Plate Electrical Connector Tip Twist the socket counterclockwise in order to remove from the lamp housing.
4 | Rear License Plate Assembly Bulb

## Rear License Plate Lamp Replacement Solstice

Callout | Component Name
--- | ---
1 | Rear License Plate Lamp Assembly Screw (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten 2 N·m (18 lb in)
2 | Rear License Plate Lamp Assembly Tip Push one side of the lamp assembly inside the rear bumper cover hole and pull downward to disconnect the electrical connector.
3 | Rear License Plate Electrical Connector Tip Twist the socket counterclockwise in order to remove from the lamp housing.
4 | Rear License Plate Bulb Tip Replace the bulb as needed.