For 1990-2009 cars

Connector 1: | Engine Coolant Level Switch
Connector 2: | Engine Cooling Fan (LE5)
Connector 3: | Engine Cooling Fan (LNF)

### Engine Coolant Level Switch

#### Connector Part Information

- OEM: 12052641
- Service: 12102747
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Engine Coolant Level Switch

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | L-GN | 1478 | Collant Level Switch Signal
B | BK/WH | 451 | Ground

### Engine Cooling Fan (LE5)

#### Connector Part Information

- OEM: 12124685
- Service: 12116243
- Description: 3-Way F Metri-Pack 630 Series, Sealed (BK)

#### Terminal Part Information

- Terminal: 15305232/23
- Core/Insulation Crimp: F/3
- Release Tool/Test Probe: J-38125-11A/J-35616-42 (RD)

#### Engine Cooling Fan (LE5)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BK | 250 | Ground
B | L-BU | 409 | Cooling Fan Motor Supply Voltage
C | GY | 532 | Cooling Fan Motor Supply Voltage

### Engine Cooling Fan (LNF)

#### Connector Part Information

- OEM: 7283-8496-30
- Service: 19115593
- Description: 4-Way F Mixed Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: Pins: 1, 2 - 7116-3250/10Pins: 4 - 7116-4110-02/9
- Core/Insulation Crimp: Pins: 1, 2 - See Terminal Repair KitPins: 4 - E/C
- Release Tool/Test Probe: Pins: 1, 2 - 12094430/J-35616-22 (RD)Pins: 4 - 12094430/J-35616-4A (PU)

#### Engine Cooling Fan (LNF)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | RD/BK | 342 | Battery Positive Voltage
2 | BK | 650 | Ground
3 | -- | -- | Not Available
4 | WH | 2368 | Cooling Fan Clutch Supply Voltage