For 1990-2009 cars

Table 1: | System Check - Without Fog Lamps
Table 2: | System Check - With Fog Lamps

#### System Check - Without Fog Lamps

ACTION | NORMAL RESULTS
--- | ---

• | Start the engine and allow to idle in PARK.

• | Neutral w/manual transaxle

• | Apply the park brake.

• | The high beam and low beam headlamps are OFF.

• | The daytime running lamps indicator is OFF.

• | Release the park brake.

• | Move the transaxle out of PARK (P) (Automatic).

• | The headlamps are ON at reduced brilliance (DRL mode).

• | The daytime running lamps indicator is ON.

• | Move the headlamp dimmer switch to LOW.

• | Turn the headlamp switch to HEAD.

• | The high beam headlamps are OFF.

• | The low beam headlamps are ON.

• | The daytime running lamps indicator is OFF.

Move the headlamp dimmer switch to HIGH. |

• | The high beam headlamps and high beam indicator are ON.

• | The low beam headlamps are OFF.

• | The daytime running lamps indicator is OFF.

Turn headlamp switch to OFF. |

• | The headlamps are ON at reduced brilliance.

• | The daytime running lamps indicator is ON during the day with the A/C OFF.

Turn the ignition switch to OFF. | The headlamps are OFF.
Move the headlamp switch to PARK. |

• | The park lamps are ON.

• | The headlamps are ON at reduced brilliance (DRL mode).

The daytime running will operate normally during the day.

#### System Check - With Fog Lamps

ACTION | NORMAL RESULTS
--- | ---

• | Start the engine and allow it to idle.

• | Move the gear selector to any position except PARK (P).

• | The fog lamp switch is OFF.

• | Apply the park brake.

• | The fog lamps, high beam headlamps, and low beam headlamps are OFF.

• | The daytime running lamps indicator is OFF.

Release the park brake. |

• | The headlamps and fog lamps are OFF.

• | The headlamps are ON at reduced brilliance (DRL mode).

• | The daytime running lamps indicator is ON.

• | Move the headlamp switch to HEAD.

• | Move the fog lamp switch ON.

• | The headlamp dimmer switch is in HIGH.

• | The high beam headlamps and high beam indicator are ON.

• | The low beam headlamps and fog lamps are OFF.

• | Move the headlamp dimmer switch to LOW.

• | Move the fog lamp switch to ON.

• | The low beam headlamps and fog lamps are ON.

• | The high beam headlamps and high beam indicator are OFF.

• | Move headlamp switch to PARK.

• | Fog lamp switch is still ON.

• | The headlamps are OFF.

• | The fog lamps are ON.

Turn the ignition switch OFF. | Headlamps and fog lamps are OFF.