For 1990-2009 cars

## License Plate Lamp Replacement SC1, SC2 Models Only

For the type of bulb required for replacement, see Replacement Bulbs .

1. Allow bulb to cool.
2. Remove the fasteners from the license plate lamp lens.
3. Gently pull the bulb from the socket straight out.
4. Replace with an appropriate bulb.

## License Plate Lamp Replacement SL, SL1, SL2 Models Only

For the type of bulb required for replacement, see Replacement Bulbs .

1. Turn off headlamp switch and allow bulb to cool before changing.
2. Remove the license plate bracket, if equipped, before you change the bulb.
3. With a small screwdriver, pry the tab on the lamp inward and pull out on the unit to release it from the compartment lid.
4. Twist the socket clockwise to release it from the lamp.
5. Replace with an appropriate bulb.