For 1990-2009 cars

### Removal Procedure

1. Remove the front bumper fascia applique upper plastic retainers.
2. Gently pull the top of the front fascia forward exposing the back of the front fascia.
3. With a screwdriver, unsnap the lower portion of the applique from the backside.

### Installation Procedure

1. Position the applique to the front fascia. Snap it into place.
2. Install the upper plastic retainers.