For 1990-2009 cars

Application | Specifications
--- | ---
Metric | English
Air Box Attachment Bolts | 10 N·m | 89 lb in
Battery Hold Down-to-Battery Tray Fasteners | 9 N·m | 80 lb in
Battery Terminal Bolts | 17 N·m | 13 lb ft
Battery Tray-to-Frame Rail Bolts | 10 N·m | 89 lb in
Brake Master Cylinder-to-Brake Booster Nuts | 27 N·m | 20 lb ft
Clutch Fork Ball Stud | 24 N·m | 18 lb ft
Clutch Housing Cover-to-Flywheel Bolts | 25 N·m | 18 lb ft
Clutch Housing-to-Engine Bolts | 140 N·m | 103 lb ft
Clutch Hydraulic Damper Bracket-to-Case Studs | 25 N·m | 18 lb ft
Clutch Pedal Pivot Shaft Attachment Nut | 17 N·m | 13 lb ft
Flywheel-to-Crankshaft Bolts (In Crisscross Pattern) | 80 N·m | 59 lb ft
I/P Upper Trim Panel Fasteners | 6 N·m | 53 lb ft
PCM Attachment Bolts | 6 N·m | 53 lb in