For 1990-2009 cars

# Service Information on New Torque Specification for Front Seat Adjuster to Vehicle Bolts

Subject: | Service Information on New Torque Specification for Front Seat Adjuster to Vehicle Bolts.

Models: | 1991 -- 1999 Saturns

### Purpose:

This bulletin provides technical information on changes to the torque specifications for front seat adjuster to vehicle bolts. The specification provided within this bulletin supercedes the specification available in prior versions of the Body/Repair Service Manuals and Quick Reference Manuals

### Correction:

Important: Bolts require Loctite ® 242 Threadlocker, P/N 21485277 (or equivalent) prior to installation.

New front seat Adjuster to vehicle bolt torque:

Tighten
Tighten bolt to 30 N·m (22 lb ft) ( Graphic SMBIS63760AG1)