For 1990-2009 cars

Application | Specifications
--- | ---
Torque Spec Description | Metric | English
Axle-to-Hub Nut | 200 N·m | 148 lb ft
Intermediate Axle Shaft Support Bracket-to-Engine Block Bolts | 54 N·m | 40 lb ft
Intermediate Axle Shaft Support Bracket-to-Intake Manifold Bracket (at Intake Manifold) | 8 N·m | 71 lb in
Intermediate Axle Shaft Support Bracket-to-Intake Manifold Bracket (at Intermediate Shaft Bracket) | 30 N·m | 22 lb ft