For 1990-2009 cars

# Replacement Sunroof Module Motor Harness Connection Changes - kw plug terminal

Subject: | Replacement Sunroof Module Motor Harness Connection Changes

Models: | .

The following diagnosis might be helpful if the vehicle exhibits the symptom described in the PI.

### Condition/Concern:

Replacement sunroof module motor harness connection does not fit in-vehicle connector.

### Recommendation/Instructions:

A second design motor/module was released for 1996 - 2002 sedans and 1997-2002 coupe vehicles. The second design motor has a pigtail wire harness instead of a fixed type connection.

When installing a second design sunroof module into a vehicle that was originally built with a first design sunroof module, a Sunroof Switch Wiring Harness Assembly, P/N 21054119, must be used to connect between the headliner harness and motor.

.

Please follow this diagnosis process thoroughly and complete each step. If the condition exhibited is resolved without completing every step, the remaining steps do not need to be performed. If these steps do not resolve the condition, please contact GM TAC for further diagnostic assistance.

### Models:

(96, 97, 98, 99, 00, 01, 02 Saturn S-Series)

.