For 1990-2009 cars

### Removal Procedure

1. Remove the ABS control assembly. Refer to Electronic Brake Control Module Replacement .
2. Remove the bolts securing the bracket to the mid-rail.

### Installation Procedure

1. Align the bracket to mid-rail, then install and torque the bolts.

Tighten
Tighten the ABS control assembly brackets bolts to 16 N·m (12 lb ft).

2. Install the ABS control assembly. Refer to Electronic Brake Control Module Replacement .