For 1990-2009 cars

# Interim Revision to the RKE/Saturn Security System Battery Feed Circuit

Subject: | Service Information on Interim Revisions to the Remote Keyless Entry/Saturn Security System (RKE/SSS) Battery Feed Circuit

Models: | 1997 Saturns

### Purpose:

On vehicles built before and including the vehicle identification numbers (VINs) shown in the chart on the next page, the battery feed circuit for the remote keyless entry/Saturn security system (RKE/SSS) is the 10 Amp BODY fuse (circuit 340). On vehicles built after and including the VINs shown in the chart on the next page, the battery feed circuit for the RKE/SSS is the 10 Amp CHIME fuse (circuit 440).

Due to this change in the battery feed circuit for the RKE/SSS, the following changes have been made to the 68-way Gray body-to-instrument panel junction block (IPJB) connector.

• | On all vehicles, circuit 340R has been moved from cavity B8 to cavity A5. This changes the circuit from 340R to 440R.

• | On wagons only, cavity A5 will also include circuit 440A for the cargo lamp.

The second edition of the 1997 Saturn Electrical Service Manual will have the updated schematics reflecting this change.

The 1997 Saturn Owner's Handbook will not be modified to show this change.

VIN Breakpoints | Body Style | Production Body Harness P/N | Usage
--- | --- | --- | ---
VZ258614 VZ264043 VZ256051 | SC SL SW | 21023307 21023300 21023299 | MIRROR-O/S, LH REM CONT, RH DIRECT CONTROL (D35), W/BASE BRK (J41) W/O RKE (AU0)
VZ280709 VZ264043 VZ258186 | SC SL SW | 21023308 21023301 21023312 | MIRROR-O/S, LH REM CONT, RH DIRECT CONTROL (D35), W/ABS W/RR DISC (JL9) OR ABS W/RR DRUM (JM4) W/O RKE (AU0)
VZ264139 VZ258361 VZ258052 | SC SL SW | 21023309 21023304 21023315 | ELEC MIR (DC0) W/BASE BRK (J41)
VZ260777 VZ256687 VZ263752 | SC SL SW | 21023310 21023305 21023316 | ELEC MIR (DC0) W/ABS W/RR DISC (JL9) OR ABS W/RR DRUM (JM4)
VZ256165 VZ262787 | SL SW | 21023302 21023313 | Mirror-- O/S, LH REM CONT, RH DIRECT CONTROL (D35), W/BASE BRK (J41) W/RKE (AU0)
VZ256768 VZ258577 | SL SW | 21023303 21023314 | Mirror--O/S, LH REM CONT, RH DIRECT CONTROL (D35), W/ABS W/RR DISC (JL9) OR ABS W/RR DRUM (JM4), W/RKE (AU0)