For 1990-2009 cars

Table 1: | Driver Inflator-1998 Only
Table 2: | Driver Inflator -- Coil Pigtail-1998 Only
Table 3: | Driver Inflator-1999 Only
Table 4: | Driver Inflatoe-Coil Pigtail-1999 Only
Table 5: | Driver Inflator-Coil Pigtail-1998 Only
Table 6: | Driver Inflator-Coil Pigtail-1999 Only
Table 7: | Driver Seat Belt Switch
Table 8: | Passenger Inflator-1998 Only
Table 9: | Passenger Inflator-1999 Only
Table 10: | Sensing and Diagnostic Module-1998 Only
Table 11: | Sensing and Diagnostic Module-1999 Only
Table 12: | Sensing and Diagnostic Module-Lamp Driver Module-1999 Only

#### Driver Inflator-1998 Only

Connector Part Information |

• | 12124324

• | Yellow

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | WHT | 347 | .50 | DRIVER SIDE HI
B | DK GRN | 348 | .50 | DRIVER SIDE LOW
Location: I/P -- Lower Left -- Base of Steering Column

#### Driver Inflator -- Coil Pigtail-1998 Only

Connector Part Information |

• | 12007568

• | Yellow/Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | WHT | 347 | .35 | DRIVER SIDE HI
B | DK GRN | 348 | .35 | DRIVER SIDE LOW
Location: Steering Wheel, Driver Inflator

#### Driver Inflator-1999 Only

Connector Part Information |

• | 12103927

• | Yellow

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | WHT | 347 | .50 | DRIVER SIDE HI
B | DK GRN | 348 | .50 | DRIVER SIDE LOW
Location: I/P -- Lower Left-Base of Steering Column

#### Driver Inflatoe-Coil Pigtail-1999 Only

Connector Part Information |

• | 97U-1005 Type C

• | Yellow

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | WHT | 347 | .35 | DRIVER SIDE HI
B | DK GRN | 348 | .35 | DRIVER SIDE LOW
Location: Steering Wheel, Driver Inflator

#### Driver Inflator-Coil Pigtail-1998 Only

Connector Part Information |

• | 12092865

• | Yellow

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | WHT | 347 | .35 | DRIVER INFLATOR HI
B | DK GRN | 348 | .35 | DRIVER INFLATOR LOW
Location: I/P-Lower Left-Base of Steering Column

#### Driver Inflator-Coil Pigtail-1999 Only

Connector Part Information |

• | 12077925

• | Yellow

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | WHT | 347 | .35 | DRIVER INFLATOR HI
B | DK GRN | 348 | .35 | DRIVER INFLATOR LOW
Location: I/P-Lower Left-Base of Steering Column

#### Driver Seat Belt Switch

Connector Part Information |

• | 12052832

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | BLK/WHT | 238A | .35 | EAT BELT SWITCH
B | BLK | 250E | .35 | GROUND
Location: Under Driover Seat-Left Front

#### Passenger Inflator-1998 Only

Connector Part Information |

• | 12110288

• | Yellow

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | DK GRN/WHT | 1404 | .50 | PASS INFLATOR LO
B | WHT/BLK | 1403 | .50 | PASS INFLATOR HI
Location: Under I/P Top Cover-Right Side

#### Passenger Inflator-1999 Only

Connector Part Information |

• | 12110505

• | Yellow

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | DK GRN/WHT | 1404 | .50 | PASS INFLATOR LO
B | WHT/BLK | 1403 | .50 | PASS INFLATOR HI
Location: Under I/P Top Cover-Right Side

#### Sensing and Diagnostic Module-1998 Only

Connector Part Information |

• | 15326054

• | Yellow

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
1 | WHT/BLK | 1403 | .50 | PASS SIDE HI
2 | WHT | 347 | .50 | DRIVER SIDE HI
3 | DK GRN | 348 | .50 | DRIVER SIDE LO
4 | DK GRN/WHT | 1404 | .50 | PASS SIDE LO
5 | TAN | 800 | .35 | SERIAL DATA (DLC)
6 | BLK/WHT | 1751 | .50 | GROPUND
7 | BRN | 358 | .35 | AIR BAG TT LAMP
8 | BLK/WHT | 238B | .35 | DRVR SEAT BELT SW
9 | -- | -- | -- | --
10 | YEL | 1139 | .35 | SIR ON & CRANK FUSE (IGN 1)
11-12 | -- | -- | -- | --
Location: Undae Console

#### Sensing and Diagnostic Module-1999 Only

Connector Part Information |

• | 15318142

• | Yellow

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A1 | YEL | 1139 | .35 | SIR ON & CRANK FUSE (IGN 1)
A2 | -- | -- | -- | --
A3 | WHT/BLK | 1403 | .50 | PASS SIDE HI
A4 | PPL | 1807 | .35 | CLASS 2 SERIAL DATA
A5 | -- | -- | -- | --
A6 | WHT | 347 | .50 | DRIVER SIDE HI
A7 | DK GRN | 348 | .50 | DRIVER SIDE LO
A8 | DK GRN/WHT | 1404 | .50 | PASS SIDE LO
A9 | LT GRN/BLK | 875 | .35 | AIR BAG TT LAMP
A10-A14 | -- | -- | -- | --
A15 | BLK/WHT | 238 | .35 | DRVR SEAT BELT SW
A16-A18 | -- | -- | -- | --
Location: Under Console

#### Sensing and Diagnostic Module-Lamp Driver Module-1999 Only

Connector Part Information |

• | 12015410

• | Green

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | BRN | 358 | .35 | AIR BAG TELLTALE
B | PNK | 39X | .35 | IGNITION
C | BRN | 875B | .35 | INPUT FROM SDM
D | BLK | 350LD | .35 | GROUND
E-F | -- | -- | -- | --
Location: Under Console