For 1990-2009 cars

Important: The spray pattern differs from side-to-side by design.

The washer nozzle spray pattern is identified in the illustration. If the nozzle is not delivering washer fluid according to the illustration, make sure that the nozzle is properly seated in the shroud top vent grille assembly.

Make sure that the top shroud vent grille assembly is installed correctly. If the spray of washer fluid still does not match the illustration, replace one or both of the washer nozzles as required.