For 1990-2009 cars

## Fender Upper Reinforcement Brace Replacement - Front Coupe

### Removal Procedure

1. Remove the front fender. Refer to Front Fender Replacement .
2. Remove the rivets that retain the brace to the spaceframe.

### Installation Procedure

1. Position the fender brace to the spaceframe and install the rivets.
2. Install the front fender. Refer to Front Fender Replacement .

## Fender Upper Reinforcement Brace Replacement - Front Sedan

### Removal Procedure

1. Remove the front fender. Refer to Front Fender Replacement .
2. Remove the rivets that retain the brace to the spaceframe.

### Installation Procedure

1. Position the fender brace to the spaceframe and install the rivets.
2. Install the front fender. Refer to Front Fender Replacement .