For 1990-2009 cars

Table 1: | Fluid and Lubricants

The following approximate capacities are given in English and metric conversions.

Fluid Changes | Capacities
--- | ---
English | Metric

#### Transaxle

- Manual (fluid change)
- Automatic (fluid change with filter)

####

- 2.6 quarts
- 4.2 quarts

####

- 2.5 L
- 4.0 L

Cooling System | 7.0 quarts | 6.6 L
Engine Crankcase (Oil and Filter) | 4 quarts | 3.8 L
Fuel Tank | 12.1 gallons | 45.8 L

#### Power Steering

- Pump Only
- Complete System

####

- 14 ounces
- 28 ounces

####

- 0.40 L
- 0.80 L

Windshield Washer Solvent (Container) | 1.0 gallon | 3.8 L
All capacities are approximate. When adding, be sure to fill to the approximate level, as recommended in this manual. Recheck fluid level after filling.

### Specifications

Engine Type | SOHC (L24), DOHC (LL0)
Engine Firing Order | 1-3-4-2
Thermostat Temperature | 194°F (90°C)
Tire Pressures and Sizes: See the Tire Loading Information Label, located on the driver's side third door, below the door striker (coupe) or rear edge of the driver's door (sedan).
Wheel Nut Torque | 140 N·m 103 ft lb

#### Fluid and Lubricants

Item | Application | Part Number | Size
--- | --- | --- | ---
DEX-COOL® (ethylene-glycol based) Antifreeze Coolant | Year-round Antifreeze Coolant Mixtures | 21031164 | 1 gal. (3.79 L)
DOT 3/Delco Supreme 11 Brake Fluid | Brake System/Clutch Hydraulic System | 21013073 or 12377967 | 16 oz. (.47 L)
Saturn Transmission Fluid or Dexron®-III | Automatic and Manual Transaxle | 21005856 | 32 oz. (.946 L)
Engine Oil SAE 5W-30 with "Starburst" Symbol | Engine Lubrication | 21007582 | 32 oz. (.95 L)
Lubricant Lubriplate® | Hood Latch Release, Pawl and Door Check Links, Sunroof Cables | 21038914 | 12 oz. (.36 L)
Power Steering Fluid | Power Steering System | 21007583 | 16 oz. (.47 L)
Washer Solvent | Windshield Washer System | 01051515 | 32 oz. (.95 L)
Silicone Grease | Weatherstrips | 18010908 | 1/4 oz.

* If used, a maintenance interval of 30,000 miles (50,000 km) must be followed for automatic transaxle fluid and filter changes.