For 1990-2009 cars

# Service Information on Counterclockwise Rotation of A/C Compressor Clutch Drive Plate

Subject: | Service Information on Counterclockwise Rotation of A/C Compressor Clutch Drive Plate

Models: | 1996 Saturns built after and including VIN TZ445870 and any vehicle serviced with the R134a service compressor (P/N 21031196)

### Purpose:

Internal changes have been made to A/C compressor built after the above mentioned VIN that allow the A/C system to rotate the A/C compressor clutch drive plate in a counterclockwise rotation, after the A/C clutch is disengaged. This counterclockwise rotation is caused by the system pressure equalizing between the high side and low side after A/C clutch disengagement, and is considered normal.

Since the time for the high and low side system pressure to equalize is determined by temperature and pressure, the A/C clutch drive plate may rotate up to two minutes after A/C clutch disengagement.