For 1990-2009 cars

Complaint/Condition | Possible Cause(s) | Correction(s)
--- | --- | ---
Clicking noise in turns | Worn or damaged outer CV joints | Replace outer CV joints
Clunk when accelerating from coast-to-drive | Worn or damaged inboard tri-pot joints | Replace inboard tri-pot joints
Shudder or vibration during acceleration | Excessive joint angle

• | Incorrect toe

• | Incorrect trim height

• | Worn or damaged inner or outer CV joints

Adjust toe

Correct trim height

Replace inner or outer CV joints

Vibration at highway speeds | Out of balance wheels or tires | Balance wheels or tires
Out of round wheels or excessive radial force variation (hard spot in tire) tires | Replace wheels or tires
Worn CV joints | Replace CV joints
Binding or tight CV joints | Replace CV joints