For 1990-2009 cars

# SMU - FOR EGR DIAGNOSTIC TROUBLE CODES

#### SUBJECT: Service Manual Update for EGR Diagnostic Trouble Codes P0401, P0404, P0405 and P1404 -------------------------------------------------------------

#### MODELS AFFECTED: 1997 Saturns -------------

#### PURPOSE

The diagnostic information for diagnostic trouble codes (DTCS) P0401, P0404, P0405 and P1404 has been updated to include additional failure modes in the EGR system.

#### IMPORTANT: When diagnosing DTCs P0401, P0404, P0405 and P1404, use the diagnostic information in this bulletin, do not use the information contained in the 1997 Powertrain Controls Service Manual.

#### IMPORTANT: When an EGR DTC P0404 or P1404 sets, some functions will be disabled for the duration of that ignition cycle. When repairs are complete, DTCs must be cleared, and ignition keyed Off for at least 10 seconds to allow proper operation.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.