For 1990-2009 cars

Table 1: | I/P Cluster
Table 2: | I/P Cluster
Table 3: | I/P Dimmer
Table 4: | I/P Junction Block-Body
Table 5: | I/P Junction Block-I/P
Table 6: | I/P Junction Block-I/P
Table 7: | Brake Switch
Table 8: | Cargo Lamp Switch-Wagon
Table 9: | Cargo Lamp-Sedan, Coupe
Table 10: | Cargo Lamp Switch-Sedan, Coupe
Table 11: | Cargo Lamp Switch-Sedan, Coupe
Table 12: | Cargo Lamp-Wagon

#### I/P Cluster

Connector Part Information |

• | 12129405

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | -- | -- | -- | --
B | PPL/WHT | 455 | .35 | FUEL GAGE SIGNAL
C | PPL | 1885 | .35 | SERVICE TT
D | BRN/WHT | 419 | .35 | MALFUNCTION INDICATOR LAMP (MIL) SERVICE ENGINE SOON
E | YEL | 172 | .35 | LOW FUEL TT
F | BRN | 358 | .50 | AIR BAG
G | PPL/WHT | 237A | .35 | SEAT BELT TT
H | PNK | 39E | .35 | IGN 1
I | LT GRN/BLK BLK | 875 350BB | .35 .50 | ABS TT-W/ ABS GROUND W/O ABS
J | DK GRN | 389 | .35 | SPEED SIGNAL
K | BLK | 350K | .35 | GROUND
L | LT GRN/BLK | 592 | .35 | DRL RELAY CONTROL
M | ORN | 1040A | .35 | BATTERY
N | PNK | 1200E | .35 | HI BEAM TT
O | DK BLU | 1201H | .35 | HEADLAMP ON INPUT
P | LT BLU/WHT | 1414 | .35 | LH TURN SIGNAL TT
Q | LT BLU | 1134 | .35 | PARK BRAKE INPUT
R | -- | -- | -- | --
Location: I/P Left Upper

#### I/P Cluster

Connector Part Information |

• | 12129406

• | Natural

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | -- | -- | -- | --
B | TAN/BLK | 456 | .35 | UPSHIFT TT-MANUAL
C | DK GRN | 35 | .35 | HOT/LO COOLANT / AUTO TRANS FLUID TEMP TT
D | DK GRN | 135 | .35 | TEMP GAGE SIGNAL
E | BLK | 350T | .50 | GROUND
F | -- | -- | -- | --
G | TAN/WHT | 33B 33CC | .35 .50 | BRAKE TT-WITH ABS BRAKE TT-NON-ABS
H | DK GRN | 44J | .35 | DIMMER RET
I | BRN | 9AJ | .35 | DIMMER CONTROL
J | DK BLU/WHT | 1415 | .35 | RH TURN SIGNAL TT
K | WHT | 121 | .35 | TACH SIGNAL INPUT
L | PNK | 39C | .35 | IGN 1
M | LT GRN | 1656 | .35 | TRACTION ACTIVE TT-TRACTION ONLY
N | BRN | 25 | .35 | BATTERY TT
O | TAN | 31 | .35 | OIL PRESSURE TT
P | -- | -- | -- | --
Q | DK GRN | 146A | .35 | LIFTGATE TT CONTROL-WAGON ONLY
R | ORN | 440G | .35 | LIFTGATE TT POWER-WAGON ONLY
Location: I/P Left Upper

#### I/P Dimmer

Connector Part Information |

• | 12064758

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | BLK | 350C | .35 | BATT
B | DK GRN | 44 | .35 | TO ILLUM BULBS
C | BRN | 9AL | .35 | TO ILLUM BULBS
Location: I/P Left Upper

#### I/P Junction Block-Body

Connector Part Information |

• | 12129592

• | Gray

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A1 | DK GRN | 19 | .80 | RIGHT REART URN LAMP
A2 | ORN | 580-SL 580A-SW 580B-SC | .50 | TO SUNROOF MODULE
A3 | BLK/WHT | 746 | .35 | DOOR AJAR SW-RT FRT
A4 | -- | -- | -- | --
A5 | PNK | 440R | .35 | RKE MODULE
A6 | PNK | 39T | .35 | EVAP VENT VALVE
A7 | -- | -- | -- | --
A8 | ORN | 340C | .35 | MIRROR SWITCH
A9 | LT BLU | 195C | .35 | RT FT DOOR LOCK SW
A10 | GRA | 295H-SW 295J-SL | .80 | RT REAR DOOR LOCK MOTOR
A11 | -- | -- | -- | --
A12 | LT BLU | 195A | .35 | LT FRONT DOOR LOCK SWITCH
B1 | YEL | 18 | 1.0 | LT REAR TURN LAMP
B2 | -- | -- | -- | --
B3 | WHT | 156A,C | .35 | DOME LAMP
B4 | -- | -- | -- | --
B5 | BLK | 293 | 2.0 | RR WINDOW DEFOG
B6 | -- | -- | -- | --
B7 | GRA | 120 | 1.0 | FUEL PUMP MOTOR
B8 | -- | -- | -- | --
B9 | ORN | 340F | .35 | MAP LIGHTS
B10 | GRA | 295C | .80 | LR DOOR LOCK MOTOR
B11 | -- | -- | -- | --
B12 | LT BLU | 195R | .35 | RKE LOCK RELAY CONTROL
C1-C2 | -- | -- | -- | --
C3 | LT BLU/BLK | 747 | .35 | LT REAR DOOR JAMB SWITCH
C4 | GRA/BLK | 745 | .35 | LT FRONT DOOR JAMB SWITCH
C5 | ORN | 340P | .35 | RT FRONT DOOR LOCK SWITCH
C6-C7 | -- | -- | -- | --
C8 | ORN | 340BB-SL 340JJ-SC | .35 | CARGO LAMP SW
C9 | ORN | 340A | .35 | DOME LAMP
C10 | GRA | 295E 295K | .80 | LF DOOR LOCK MOTOR-SC LF DOOR LOCK MOTOR-SL,SW
C11 | -- | -- | -- | --
C12 | GRA | 295F 295B | .80 | RF DOOR LOCK MOTOR-SC RF DOOR LOCK MOTOR-SL,SW
D1-D2 | -- | -- | -- | --
D3 | LT GRN/BLK | 748 | .35 | LT FRONT DOOR JAMB SWITCH-SL,SW
D4 | -- | -- | -- | --
D5 | ORN | 340N | .35 | LT FRONT DOOR LOCK SWITCH
D6-D11 | -- | -- | -- | --
D12 | WHT | 194A | .35 | LT FRONT DOOR LOCK SWITCH
E1 | BRN | 9H-SL 9Y-SW 9P-SC | .35 | LICENSE LAMPS
E2 | BRN | 9F-SL,SC | .35 | TAIL/MARKER LAMP
E3-E8 | -- | -- | -- | --
E9 | WHT | 194R | .35 | RKE UNLOCK RELAY CONTROL
E10 | TAN | 294F-SC 294B-SL,SW | .80 | LF DOOR LOCK MOTOR LF DOOR LOCK MOTOR
E11 | BLK | 550A | .80 | GROUND
E12 | WHT | 194C | .35 | RT FRONT DOOR LOCK SWITCH
F1 | BRN | 9-SW 9R-SL | .35 | LICENSE LAMPS
F2 | BRN | 9G-SL,SC 9Z-SW | .35 | TAIL/MARKER LAMPS
F3-F8 | -- | -- | -- | --
F9 | PPL | 638-SL,SW 638C-SC | 2.0 | POWER WINDOW SWITCH
F10 | TAN | 294H-SW 294JSL | .80 | RR DOOR LOCK MOTOR
F11 | -- | -- | -- | --
F12 | TAN | 294C-SL,SW | .80 | LR DOOR LOCK MOTOR

#### I/P Junction Block-I/P

Connector Part Information |

• | 12146036

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A1 | BLK | 350N | 2.0 | I/P SPLICE PACK #1-GROUND
A2 | -- | -- | -- | --
A3 | BRN | 9J | .35 | PARK LAMPS
A4 | ORN | 340L | .35 | BODY FUSE
A5 | -- | -- | -- | --
A6 | PNK | 39X | -- | SDM TT--1999 ONLY
A7 | BRN | 9K | .35 | PARK LAMPS
A8 | BRN | 9AJ | .35 | MIRROR SWITCH
A9 | ORN | 1240 | 2.0 | REAR DEFOG RELAY
A10 | RED | 302 | 2.0 | WINDOW RELAY
A11-A12 | -- | -- | -- | --
B1 | -- | -- | -- | --
B2 | RED | 458 | 3.0 | TRS LP, TRS 2/TCC, TRS 3/4 FUSES-AUTO
B3 | BRN | 9AC 9AN | .35 | CHIME MODULE-ASH TRAY ILL. CHIME MODULE
B4-B6 | -- | -- | -- | --
B7 | BRN | 9AB 9AK | .35 .35 | HVAC ILL. CIGAR LIGHTER
B8 | BRN | 9AF | .35 | PRNDL
B9-B12 | -- | -- | -- | --
C1 | -- | -- | -- | --
C2 | DK GRN/WHT | 465 | .35 | FUEL PUMP RELAY
C3 | BRN | 9AP 9AL | .35 | CHIME MODULE-HVAC ILL CHIME MODULE-DIMMER
C4 | PPL/WHT | 237A | .35 | SEAT BELT TT
C5 | ORN | 740B | .80 | CIGAR LIGHTER
C6-C7 | -- | -- | -- | --
C8 | PNK | 39C | .35 | IGN 1 FUSE
C9 | BRN | 341B | .35 | CRUISE ENABLE SWITCH
C10 | BRN | 41 | .50 | TO BRAKE SW
C11 | PNK | 139 | 1.0 | TURN FUSE
C12 | YEL | 43 | .35 | RADIO FUSE
D1 | RED | 102B | 3.0 | HVAC BLOWER HI
D2 | -- | -- | -- | --
D3 | BRN | 9M | .35 | CHIME MODULE
D4-D7 | -- | -- | -- | --
D8 | PNK | 39E | .35 | IGN 1 FUSE
D9 | BRN | 341C | .35 | CRUISE CONTROL MODULE IGNITION FEED
D10-D12 | -- | -- | -- | --
E1 | DK BLU | 101 | .35 | BLOWER RESISTOR
E2 | BLK/WHT | 238B | .35 | CHIME MODULE
E3 | BLK/WHT | 238A | .35 | DRIVER SEAT BELT
E4 | -- | -- | -- | --
E5 | ORN | 440F 440G-WAGON | .35 | CHIME FUSE
E6 | -- | -- | -- | --
E7 | BRN | 641B | .35 | IGN 3 FUSE
E8 | BRN | 641E | .35 | IGN 3 FUSE
E9 | -- | -- | -- | --
E10 | BRN | 641A | .35 | IGN 3 FUSE
E11 | YEL | 1139 | .35 | AIR BAG FUSE
E12 | YEKL | 143 | 1.0 | WIPER FUSE
F1 | ORN | 52 | .50 | BLOWER H
F2 | PPL | 65 | 3.0 | BLOWER MOTOR
F3-F4 | -- | -- | -- | --
F5 | RED | 402 | 3.0 | CHIME/LOCKS/BODY FUSES
F6 | PNK | 139H | .35 | BRAKE PEDAL SWITCH
F7 | -- | -- | -- | --
F8 | BRN | 341F | .35 | CRUISE FUSE BRAKE PEDAL SWITCH
F9 | ORN | 300 | 3.0 | IGN 3/ CRUISE/HVAC FUSES
F10 | PNK | 3B | 2.0 | AIR BAG/TURN/IGN 1 FUSES
F11 | PNK | 3C | 2.0 | AIR BAG/TURN/IGN 1 FUSES
F12 | BRN | 4 | 2.0 | WIPER AND RADIO FUSE

#### I/P Junction Block-I/P

Connector Part Information |

• | 12129535

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A1 | TAN/WHT | 33E | .35 | ABS CONTROLLER
A2 | -- | -- | -- | --
A3 | TAN/WHT | 33C | .50 | ABS LOW BRAKE FLUID SW
A4 | TAN/WHT | 33B | .35 | ABS BRAKE TT
A5 | DK GRN | 19A | 1.0 | RR STOP/TURN LAMP
A6 | DK BLU | 15A | .50 | RF TURN SIGNAL LAMP
B1 | DK GRN | 44 44A | .35 | DIMMER ASH TRAY
B2 | DK GRN | 44F | .35 | PRNDL LAMP
B3 | DK GRN | 44J 44P | .35 | CLUSTER ILL. HVAC ILL.
B4 | DK GRN | 44L 44H | .35 | POD SW ILL. RADIO ILL.
B5 | DK GRN | 44K 44B | .35 | CIGAR LTR ILL. HVAC ILL.
B6 | DK BLU/WHT | 1415 | .35 | RF TURN SIGNAL SW
C1 | ORN | 580D | .35 | WIPER-SW
C2 | -- | -- | -- | --
C3 | LT BLU | 292 | .35 | RR DEFOG ON/OFF SWITCH
C4 | LT BLU/WHT | 1414 | .35 | LF TURN SIGNAL SW
C5 | LT BLU | 14A | .50 | LF TURN SIGNAL LAMP
C6 | YEL | 18A | 1.0 | LR STOP/TURN LAMP
D1 | -- | -- | -- | --
D2 | LT BLU | 1508B | .80 | TURN/HAZARD MODULE
D3 | -- | -- | -- | --
D4 | PPL | 16 | 1.0 | TURN SIGNAL FLASHER
D5 | LT GRN | 80 | .35 | KEY MINDER SWITCH SIGNAL
D6 | WHT | 193 | .35 | REAR DEFOG RELAY

#### Brake Switch

Connector Part Information |

• | 12092371

• | Gray

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | ORN | 540 | .50 | B+ FROM BRAKE FUSE
B | LT BLU | 20G | .50 | ABS-CONTROLLER
C | BRN BRN | 86A 86B | .35 .35 | CRUISE CONT MOD PCM
D | DK GRN/WHT | 1135 | .35 | BTSI SOLENOID
Location: Brake Pedal

#### Cargo Lamp Switch-Wagon

Connector Part Information |

• | 12052832

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | DK GRN | 146B | .35 | AJAR TELLTALE/CARGO LAMP CONTROL
B | BLK | 550AX | .35 | GROUND
Location: Liftgate Latch

#### Cargo Lamp-Sedan, Coupe

Connector Part Information |

• | 12052832

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | RED/BLK | 744 744B | .35 | GROUND-SL GROUND-SC
B | ORN | 340B 340JJ | .35 | POWER-SL POWER-SC
Location: Under Package Shelf

#### Cargo Lamp Switch-Sedan, Coupe

Connector Part Information |

• | 12047781

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | BLK | 550RA 550RL | .35 | DECKLID RELEASE MOTOR GROUND-SL W/RKE DECKLID RELEASE MOTOR GROUND-SC W/RKE
B | GRA | 382B 382C | .35 | DECKLID RELEASE MOTOR-SL W/RKE DECKLID RELEASE MOTOR-SC W/RKE
C | RED/BLK | 744A 744C | .35 | CARGO LAMP SW-SL CARGO LAMPSW-SC
Location: Decklid Latch

#### Cargo Lamp Switch-Sedan, Coupe

Connector Part Information |

• | 12092582

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | BLK | 550DD-SL 550DY-SC | .35 .80 | GROUND-SL GROUND-SC
Location: On Decklid Latch

#### Cargo Lamp-Wagon

Connector Part Information |

• | 12047781

• | Black

Cavity | Wire Color | Circuit Number | Wire Size | Circuit Function
--- | --- | --- | --- | ---
A | WHT | 156A | .35 | CARGO LP SWITCH
B | BLK | 550A | .35 | CARGO LP GROUND
C | ORN | 340A | .35 | CARGO LP BULB
Location: Rear Roof