For 1990-2009 cars

# ( DRL ) Logic Location - Assists with Proper Part Number Replacement - kw lamp light inoperative speedometer instrument panel cluster IPC IP part head

Subject: | (DRL) Logic Location - Assists with Proper Part Number Replacement

Models: | .

The following diagnosis might be helpful if the vehicle exhibits the symptom(s) described in the PI.

### Condition/Concern:

DRLs may be inoperative requiring part replacement. Described below are the locations of the DRL logic based on model year.

### Recommendation/Instructions:

DRL Logic Location:

1996 mechanical - I/P cluster housing (gauges removable - YES)

1997, 1998 mechanical - speedometer/odometer head

1998, 1999 digital - I/P cluster assembly (gauges removable - NO)

.

Please follow this diagnosis process thoroughly and complete each step. If the condition exhibited is resolved without completing every step, the remaining steps do not need to be performed.

### Models:

(1996-1999 Saturn S-Series)

.