For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
ABS Control Assembly Brackets Bolts | 16 N·m | 12 lb ft
ABS Control Assembly-to-Midrail Bracket Bolt | 12 N·m | 9 lb ft
Battery Retainer Nut Screw | 9 N·m | 80 lb in
Bleeder Screws - Front | 11 N·m | 8 lb ft
Bleeder Screws - Rear | 7.5 N·m | 66 lb in
Booster-to-Body Nuts | 27 N·m | 20 lb ft
Brake Caliper Lock Pin | 36 N·m | 27 lb ft
Brake Caliper-to-Steering Knuckle | 110 N·m | 81 lb ft
Brake Hose-to-Brake Caliper | 49 N·m | 36 lb ft
Brake Hose-to-Brake Pipe | 15 N·m | 11 lb ft
Brake Hose-to-Wheel Cylinder | 49 N·m | 36 lb ft
Brake Pedal Pivot Bolt | 22 N·m | 16 lb ft
Brake Pipe-to-ABS Assembly | 32 N·m | 24 lb ft
Brake Pipe-to-Master Cylinder Nut | 32 N·m | 24 lb ft
Control Module-to-Valve Assembly Screws | 4-6 N·m | 35-53 lb in
Front Brake Bleeder Valve | 11 N·m | 8 lb ft
Front Console Screw | 2.5 N·m | 22 lb in
Lock/Guide Pin-to-Brake Caliper | 36 N·m | 27 lb ft
Master Cylinder-to-Brake Booster Nut | 27 N·m | 20 lb ft
Negative Battery Cable | 17 N·m | 13 lb ft
PCM Attachment Bolts | 6 N·m | 53 lb in
Park Brake Lever Assembly-to-Floor | 25 N·m | 18 lb ft
Park Brake Switch Screw | 4 N·m | 35 lb in
Positive Battery Cable | 17 N·m | 13 lb ft
Rear Brake Bleeder Valve | 7.5 N·m | 66 lb in
Rear Console Screw | 2.5 N·m | 22 lb in
Rear Wheel Hub Assembly | 85 N·m | 63 lb ft
Stop Lamp Switch Mounting Nut | 10 N·m | 89 lb in
Trailing Arm/Park Brake Cable-to-Body | 120 N·m | 89 lb ft
Wheel Cylinder-to-Backing Plate | 10 N·m | 89 lb in
Wheel Nut | 140 N·m | 103 lb ft
Wheel Speed Sensor | 10 N·m | 89 lb in